{"text_format":"3","workbook":"xls","n_sheets":41,"sheets":["封面","项目总价表","1#、2#管护用房-采暖","1#、2#管护用房-电气","1#、2#管护用房-给排水","1#、2#加药间-采暖","1#、2#加药间-电气","1#、2#加药间-给排水","1#、2#污水处理厂房-采暖","1#、2#污水处理厂房-电气","1#、2#污水处理厂房-给排水","办公楼-采暖","办公楼-电气","办公楼-给排水","磅房-采暖","磅房-电气","磅房-给排水","库房-电气","库房-给排水","门卫-采暖","门卫-电气","门卫-给排水","热泵间-采暖","热泵间-电气","热泵间-给排水","修理车间-采暖","修理车间-电气","修理车间-给排水","预留用房-采暖","预留用房-电气","预留用房-给排水","原水提升泵房-采暖","原水提升泵房-电气","综合水池及泵房-采暖","综合水池及泵房-电气","综合水池及泵房-给排水","综合用房-采暖","综合用房-电气","综合用房-给排水","室外-电气工程","室外-给排水工程"],"not_rendered":{"external_links":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"封面","index":0,"n_rows":14,"n_cols":5,"rows_kept":14,"merged":[[3,0,3,8],[11,1,11,2],[11,3,11,7],[12,1,12,2],[12,3,12,7],[13,1,13,2],[13,3,13,7]],"flags":["formulas_cached_only"]}
[]
[]
[]
["年处理200万吨工业污水、油田污水、一般固体废物     处理处置项目给排水、电气、采暖\n安装劳务投标文件"]
[]
[]
[{"$nulls":4},"报"]
[{"$nulls":4},"价"]
[{"$nulls":4},"表"]
[]
[]
[null,"项目名称：",null,"                                                                                "]
[null,"投标单位：",null,"                                                                                "]
[null,"日    期：",null,"     年    月     日   "]

{"sheet":"项目总价表","index":1,"n_rows":59,"n_cols":6,"rows_kept":59,"merged":[[0,0,0,5],[56,0,56,5]],"flags":["formulas_cached_only"]}
["年处理200万吨工业污水、油田污水、一般固体废物处理处置项目\n给排水、电气、采暖安装劳务报价总表 "]
["序号","名称","建筑面积（m²）","报价（元）","单方报价（元/m²）","备注"]
[1,"1#、2#管护用房",162.5,0,0]
[1.1,"采暖",{"v":162.5,"d":"162.50"},0,0]
[1.2,"电气",{"v":162.5,"d":"162.50"},0,0]
[1.3,"给排水",{"v":162.5,"d":"162.50"},0,0]
[2,"1#、2#加药间",446.5,0,0]
[2.1,"采暖",{"v":446.5,"d":"446.50"},null,0]
[2.2,"电气",{"v":446.5,"d":"446.50"},null,0]
[2.3,"给排水",{"v":446.5,"d":"446.50"},null,0]
[3,"1#、2#污水处理厂房",{"v":5766.9,"d":"5766.90"},0,0]
[3.1,"采暖",{"v":5766.9,"d":"5766.90"},null,0]
[3.2,"电气",{"v":5766.9,"d":"5766.90"},null,0]
[3.3,"给排水",{"v":5766.9,"d":"5766.90"},null,0]
[4,"办公楼",1379.64,0,0]
[4.1,"采暖",1379.64,null,0]
[4.2,"电气",1379.64,null,0]
[4.3,"给排水",1379.64,null,0]
[5,"磅房",{"v":74.5,"d":"74.50"},0,0]
[5.1,"采暖",{"v":74.5,"d":"74.50"},null,0]
[5.2,"电气",{"v":74.5,"d":"74.50"},null,0]
[5.3,"给排水",{"v":74.5,"d":"74.50"},null,0]
[6,"库房",226.16,0,0]
[6.1,"电气",226.16,null,0]
[6.2,"给排水",226.16,null,0]
[7,"门卫",41.61,0,0]
[7.1,"采暖",41.61,null,0]
[7.2,"电气",41.61,null,0]
[7.3,"给排水",41.61,null,0]
[8,"热泵间",292.41,0,0]
[8.1,"采暖",292.41,null,0]
[8.2,"电气",292.41,null,0]
[8.3,"给排水",292.41,null,0]
[9,"修理车间",889.22,0,0]
[9.1,"采暖",889.22,null,0]
[9.2,"电气",889.22,null,0]
[9.3,"给排水",889.22,null,0]
[10,"预留用房",857.58,0,0]
[10.1,"采暖",857.58,null,0]
[10.2,"电气",857.58,null,0]
[10.3,"给排水",857.58,null,0]
[11,"原水提升泵房",108.55,0,0]
[11.1,"采暖",108.55,null,0]
[11.2,"电气",108.55,null,0]
[12,"综合水池及泵房",207.08,0,0]
[12.1,"采暖",207.08,null,0]
[12.2,"电气",207.08,null,0]
[12.3,"给排水",207.08,null,0]
[13,"综合用房",1091.63,0,0]
[13.1,"采暖",1091.63,null,0]
[13.2,"电气",1091.63,null,0]
[13.3,"给排水",1091.63,null,0]
[14,"室外工程",null,0]
[14.1,"电气"]
[14.2,"给排水"]
[15,"报价合计",null,0]
["备注：1.所有做法以图纸、图集、技术及质量标准为准予以报价；且允许报价单位自行添加或补充清单项，无增加或补充的均视为已综合到其他报价内，后期不再以调价、变更或签证方式调整价格图纸、图集做法为准，图纸范围内的漏项视为已综合在其它分项中。\n     2.以上费用均综合考虑了人工、机具、辅材、管理费、利润、风险、调试费用、安全文明费用、措施费用及多次搬运费用、税金、食宿及保险等费用。\n     3.不含通风、消防工程。\n"]
[{"$nulls":3},"投标单位（签章）："]
[{"$nulls":3},"日       期：","  年     月      日"]

{"sheet":"1#、2#管护用房-采暖","index":2,"n_rows":17,"n_cols":16,"rows_kept":17,"merged":[[0,0,0,15],[1,0,1,2],[1,4,1,14],[4,3,5,3],[6,3,9,3],[10,3,12,3],[16,0,16,13]],"flags":["formulas_cached_only"]}
["工程量清单报价表"]
["工程名称：1#、2#管护用房-采暖"]
["序号","项目名称","项目特征描述","工作内容","单位","工程量","人工费（元）","辅材费（元）","机械费（元）","管理费（元）","利润（元）","不含税单价（元）","税率（3%）","含税单价\n（元）","含税合价\n（元）","备注"]
[null,null,"示意",null,"m",1,"A","B","C","D","E","F=A+B+C+D+E","G=F*3%","H=F+G","I=H*1"]
[1,"镀锌钢管","1.材质、规格:热镀锌钢管 DN20","1.管道安装\n2.管件制作、安装\n3.压力试验\n4.吹扫、冲洗\n5.警示带铺设","m"]
[2,"镀锌钢管","1.材质、规格:热镀锌钢管 DN25",null,"m"]
[3,"螺纹阀门","1.材质、规格:温控阀 DN20","1.安装\n2.电气接线\n3.调试","个"]
[4,"螺纹阀门","1.材质、规格:截止阀J11T-10 DN20",null,"个"]
[5,"螺纹阀门","1.材质、规格:排气阀 DN20",null,"个"]
[6,"螺纹阀门","1.材质、规格:手动调节阀 DN25",null,"个"]
[7,"钢制散热器","1.材质、规格:钢制散热器（UR7002-600）8片","1.安装\n2.托架安装\n3.托架刷油","组"]
[8,"钢制散热器","1.材质、规格:钢制散热器（UR7002-600）18片",null,"组"]
[9,"钢制散热器","1.材质、规格:钢制散热器（UR7002-600）25片",null,"组"]
[10,"热力入口装置","1.名称、规格：热力入口装置","1.安装\n2.调试","套"]
[11,"技工","工程量暂定1工日",null,"工日",1]
[12,"普工","工程量暂定1工日",null,"工日",1]
["报价合计",{"$nulls":13},0]

{"sheet":"1#、2#管护用房-电气","index":3,"n_rows":16,"n_cols":16,"rows_kept":16,"merged":[[0,0,0,15],[1,0,1,2],[1,4,1,7],[4,3,5,3],[6,3,7,3],[8,3,10,3],[11,3,14,3],[15,0,15,13]],"flags":["formulas_cached_only"]}
["工程量清单报价表"]
["工程名称：1#、2#管护用房-电气"]
["序号","项目名称","项目特征描述","工作内容","单位","工程量","人工费（元）","辅材费（元）","机械费（元）","管理费（元）","利润（元）","不含税单价（元）","税率（3%）","含税单价\n（元）","含税合价\n（元）","备注"]
[1,"配电箱","1.名称、型号:AL201-600*500*100","1.本体安装\n2.基础型钢制作、安装\n3.焊、压接线端子\n4.补刷（喷)油漆\n5.接地","台"]
[2,"配线","1.名称、型号:ZR-BV2.5","1.配线\n2.钢索架设（拉紧装置安装）\n3.支持体（夹板、绝缘子、槽板等)安装","m"]
[3,"配线","1.名称、型号:ZR-BV4",null,"m"]
[4,"配管","1.名称、型号:PVC20","1.电线管路敷设\n2.钢索架设（拉紧装置安装）\n3.预留沟槽\n4.接地","m"]
[5,"配管","1.名称、型号:PVC25",null,"m"]
[6,"普通灯具","1.名称、型号:防水防尘吸顶灯-220V 1X18W","1.本体安装","套"]
[7,"装饰灯","1.名称、型号:室外雨棚灯-LED 18W  IP67W",null,"套"]
[8,"装饰灯","1.名称、型号:双管节能荧光灯-~220V 2X30W",null,"套"]
[9,"小电器","1.名称、型号:单联单控开关","1.本体安装\n2.焊、压接线端子\n3.接线","个"]
[10,"小电器","1.名称、型号:二、三极安全型插座",null,"个"]
[11,"小电器","1.名称、型号:空调插座",null,"个"]
[12,"小电器","1.名称、型号:双联单控开关",null,"个"]
["报价合计",{"$nulls":13},0]

{"sheet":"1#、2#管护用房-给排水","index":4,"n_rows":21,"n_cols":16,"rows_kept":21,"merged":[[0,0,0,15],[1,0,1,2],[1,4,1,7],[3,3,5,3],[8,3,10,3],[12,3,13,3],[14,3,15,3],[18,3,19,3],[20,0,20,13]],"flags":["formulas_cached_only"]}
["工程量清单报价表"]
["工程名称：1#、2#管护用房-给排水"]
["序号","项目名称","项目特征描述","工作内容","单位","工程量","人工费（元）","辅材费（元）","机械费（元）","管理费（元）","利润（元）","不含税单价（元）","税率（3%）","含税单价\n（元）","含税合价\n（元）","备注"]
[1,"螺纹阀门","1.名称、规格：截止阀 DN25","1.安装\n2.电气接线\n3.调试","个"]
[2,"螺纹阀门","1.名称、规格：闸阀 DN25",null,"个"]
[3,"螺纹阀门","1.名称、规格：止回阀 DN25",null,"个"]
[4,"其他成品卫生器具","1.名称、规格：地漏 DN50","1.器具安装\n2.附件安装","组"]
[5,"热水器、开水炉","1.名称、规格：电热水器","1.安装\n2.附件安装","台"]
[6,"塑料管","1.名称、规格：PPR DN15","1.管道安装\n2.管件安装\n3.塑料卡固定\n4.压力试验\n5.吹扫、冲洗\n6.警示带铺设","m"]
[7,"复合管","1.名称、规格：内涂塑钢管（内涂聚乙烯PE) DN20",null,"m"]
[8,"复合管","1.名称、规格：内涂塑钢管（内涂聚乙烯PE) DN25",null,"m"]
[9,"淋浴器","1.名称、规格：淋浴器","1.器具安装\n2.附件安装","套"]
[10,"铸铁管","1.名称、规格:柔性机制抗震铸铁管 DN100","1.管道安装\n2.管件安装\n3.压力试验\n4.吹扫、冲洗\n5.警示带铺设","m"]
[11,"铸铁管","1.名称、规格:柔性机制抗震铸铁管 DN50",null,"m"]
[12,"塑料管","1.名称、规格：热水 PPR DN15","1.管道安装\n2.管件安装\n3.塑料卡固定\n4.阻火圈安装\n5.压力试验\n6.吹扫、冲洗\n7.警示带铺设","m"]
[13,"塑料管","1.名称、规格：热水 PPR DN20",null,"m"]
[14,"水表","1.名称、规格：水表 DN25","1.组装","组"]
[15,"套管","1.名称、规格：刚性防水套管 DN40","1.制作\n2.安装\n3.除锈、刷油","个"]
[16,"洗脸盆","1.名称、规格：台式洗脸盆","1.器具安装\n2.附件安装","组"]
[17,"大便器","1.名称、规格：坐便",null,"组"]
["报价合计",{"$nulls":13},0]

{"sheet":"1#、2#加药间-采暖","index":5,"n_rows":12,"n_cols":16,"rows_kept":12,"merged":[[0,0,0,15],[1,0,1,2],[1,4,1,7],[3,3,5,3],[6,3,9,3],[11,0,11,13]],"flags":["formulas_cached_only"]}
["工程量清单报价表"]
["工程名称：1#、2#加药间-采暖"]
["序号","项目名称","项目特征描述","工作内容","单位","工程量","人工费（元）","辅材费（元）","机械费（元）","管理费（元）","利润（元）","不含税单价（元）","税率（3%）","含税单价\n（元）","含税合价\n（元）","备注"]
[1,"镀锌钢管","1.材质、规格:热镀锌钢管 DN20","1.管道安装\n2.管件制作、安装\n3.压力试验\n4.吹扫、冲洗\n5.警示带铺设","m"]
[2,"镀锌钢管","1.材质、规格:热镀锌钢管 DN25",null,"m"]
[3,"镀锌钢管","1.材质、规格:热镀锌钢管 DN32",null,"m"]
[4,"螺纹阀门","1.材质、规格:温控阀 DN20","1.安装\n2.电气接线\n3.调试","个"]
[5,"螺纹阀门","1.材质、规格:截止阀J11T-10 DN20",null,"个"]
[6,"螺纹阀门","1.材质、规格:排气阀 DN20",null,"个"]
[7,"螺纹阀门","1.材质、规格:手动调节阀 DN32",null,"个"]
[8,"钢制散热器","1.材质、规格:钢制散热器（UR7002-600）14片","1.安装\n2.托架安装\n3.托架刷油","组"]
["报价合计",{"$nulls":13},0]

{"sheet":"1#、2#加药间-电气","index":6,"n_rows":25,"n_cols":16,"rows_kept":25,"merged":[[0,0,0,15],[1,0,1,2],[1,4,1,7],[4,3,7,3],[16,3,17,3],[20,3,22,3],[24,0,24,13]],"flags":["formulas_cached_only"]}
["工程量清单报价表"]
["工程名称：1#、2#加药间-电气"]
["序号","项目名称","项目特征描述","工作内容","单位","工程量","人工费（元）","辅材费（元）","机械费（元）","管理费（元）","利润（元）","不含税单价（元）","税率（3%）","含税单价\n（元）","含税合价\n（元）","备注"]
[null,"动力部分"]
[1,"配电箱","1.名称、型号:加药间照明配电箱 DZ30-12","1.本体安装\n2.基础型钢制作、安装\n3.焊、压接线端子\n4.补刷（喷)油漆\n5.接地","台"]
[2,"配电箱","1.名称、型号:加药间应急照明配电箱\n2.规格:400*500*200",null,"台"]
[3,"配电箱","1.名称、型号:加药间检修配电箱 JXF 405020",null,"台"]
[4,"配电箱","1.名称、型号:加药间风机配电箱 JXF405020 0.5kW",null,"台"]
[5,"电缆槽盒","1.名称、型号:镀锌槽式电缆桥架 300X100","1.槽盒安装","m"]
[6,"电力电缆","1.名称、型号:YJV-4x2.5","1.电缆敷设\n2.揭（盖）盖板","m"]
[null,"照明部分"]
[7,"装饰灯","1.名称、型号:LED投光灯-LED 防尘防水型 40W","1.本体安装","套"]
[8,"装饰灯","1.名称、型号:天棚灯-LED 18W",null,"套"]
[9,"小电器","1.名称、型号:单联开关-86K31-10","1.本体安装\n2.焊、压接线端子\n3.接线","个"]
[10,"小电器","1.名称、型号:双联开关-86K21-10",null,"个"]
[11,"配线","1.名称、型号:ZR-BV4","1.配线\n2.钢索架设（拉紧装置安装）\n3.支持体（夹板、绝缘子、槽板等)安装","m"]
[12,"配管","1.名称、型号:PVC25","1.电线管路敷设\n2.钢索架设（拉紧装置安装）\n3.预留沟槽\n4.接地","m"]
[13,"配管","1.名称、型号:SC25",null,"m"]
[null,"防雷接地"]
[14,"配电箱","1.名称、型号:等电位端子箱 TD28","1.本体安装\n2.基础型钢制作、安装\n3.焊、压接线端子\n4.补刷（喷)油漆\n5.接地","台"]
[15,"接地母线","1.名称、型号:镀锌扁钢接地线 -40X4","1.接地母线制作、安装\n2.补刷（喷)油漆","m"]
[16,"接地母线","1.名称、型号:接地保护连接线 -25X4 镀锌扁铁",null,"m"]
[17,"接地母线","1.名称、型号:接地保护连接线 -40X4 不锈钢扁铁",null,"m"]
[18,"接地极","1.名称、型号:接地极-Φ50镀锌钢管长2500MM","1.接地极（板、桩)制作、安装\n2.基础接地网安装\n3.补刷（喷)油漆","根"]
["报价合计",{"$nulls":13},0]

{"sheet":"1#、2#加药间-给排水","index":7,"n_rows":13,"n_cols":16,"rows_kept":13,"merged":[[0,0,0,15],[1,0,1,2],[1,4,1,7],[3,3,5,3],[12,0,12,13]],"flags":["formulas_cached_only"]}
["工程量清单报价表"]
["工程名称：1#、2#加药间-给排水"]
["序号","项目名称","项目特征描述","工作内容","单位","工程量","人工费（元）","辅材费（元）","机械费（元）","管理费（元）","利润（元）","不含税单价（元）","税率(3%)","含税单价\n（元）","含税合价\n（元）","备注"]
[1,"螺纹阀门","1.名称、规格：截止阀 DN40","1.安装\n2.电气接线\n3.调试","个"]
[2,"螺纹阀门","1.名称、规格：闸阀 DN40",null,"个"]
[3,"螺纹阀门","1.名称、规格：倒流器 DN40",null,"个"]
[4,"其他成品卫生器具","1.名称、规格：地漏 DN100","1.器具安装\n2.附件安装","组"]
[5,"热水器、开水炉","1.名称、规格：电热水器","1.安装\n2.附件安装","台"]
[6,"复合管","1.名称、规格：内涂塑钢管（内涂聚乙烯PE) DN40","1.管道安装\n2.管件安装\n3.塑料卡固定\n4.压力试验\n5.吹扫、冲洗\n6.警示带铺设","m"]
[7,"铸铁管","1.名称、规格:柔性机制抗震铸铁管 DN100","1.管道安装\n2.管件安装\n3.压力试验\n4.吹扫、冲洗\n5.警示带铺设","m"]
[8,"水表","1.名称、规格：水表 DN40","1.组装","组"]
[9,"套管","1.名称、规格：刚性防水套管 DN40","1.制作\n2.安装\n3.除锈、刷油","个"]
["报价合计",{"$nulls":13},0]

{"sheet":"1#、2#污水处理厂房-采暖","index":8,"n_rows":16,"n_cols":16,"rows_kept":16,"merged":[[0,0,0,15],[1,0,1,2],[1,4,1,7],[3,3,8,3],[9,3,12,3],[15,0,15,13]],"flags":["formulas_cached_only"]}
["工程量清单报价表"]
["工程名称：1#、2#污水处理厂房-采暖"]
["序号","项目名称","项目特征描述","工作内容","单位","工程量","人工费（元）","辅材费（元）","机械费（元）","管理费（元）","利润（元）","不含税单价（元）","税率（3%）","含税单价\n（元）","含税合价\n（元）","备注"]
[1,"镀锌钢管","1.材质、规格:热镀锌钢管 DN25","1.管道安装\n2.管件制作、安装\n3.压力试验\n4.吹扫、冲洗\n5.警示带铺设","m"]
[2,"镀锌钢管","1.材质、规格:热镀锌钢管 DN32",null,"m"]
[3,"镀锌钢管","1.材质、规格:热镀锌钢管 DN40",null,"m"]
[4,"镀锌钢管","1.材质、规格:热镀锌钢管 DN50",null,"m"]
[5,"镀锌钢管","1.材质、规格:热镀锌钢管 DN65",null,"m"]
[6,"镀锌钢管","1.材质、规格:热镀锌钢管 DN80",null,"m"]
[7,"螺纹阀门","1.材质、规格:手动调节阀 DN20","1.安装\n2.电气接线\n3.调试","个"]
[8,"螺纹阀门","1.材质、规格:闸阀 DN20",null,"个"]
[9,"螺纹阀门","1.材质、规格:自动排气阀 DN20",null,"个"]
[10,"螺纹阀门","1.材质、规格:70°防火阀",null,"个"]
[11,"热力入口装置","1.名称、规格：热力入口装置","1.安装\n2.调试","套"]
[12,"钢制散热器","1.材质、规格:钢制散热器（UR7002-600）25片","1.安装\n2.托架安装\n3.托架刷油","组"]
["报价合计",{"$nulls":13},0]

{"sheet":"1#、2#污水处理厂房-电气","index":9,"n_rows":79,"n_cols":16,"rows_kept":79,"merged":[[0,0,0,15],[1,0,1,2],[1,4,1,7],[4,3,11,3],[12,3,17,3],[22,3,25,3],[26,3,42,3],[44,3,54,3],[55,3,58,3],[59,3,60,3],[61,3,69,3],[73,3,75,3],[78,0,78,13]],"flags":["formulas_cached_only"]}
["工程量清单报价表"]
["工程名称：1#、2#污水处理厂房-电气"]
["序号","项目名称","项目特征描述","工作内容","单位","工程量","人工费（元）","辅材费（元）","机械费（元）","管理费（元）","利润（元）","不含税单价（元）","税率(3%)","含税单价\n（元）","含税合价\n（元）","备注"]
[null,"动力部分"]
[1,"配电箱","1.名称、型号:1#处理厂房应急照明配电箱\n2.规格:500*600*200","1.本体安装\n2.基础型钢制作、安装\n3.焊、压接线端子\n4.补刷（喷)油漆\n5.接地","台"]
[2,"配电箱","1.名称、型号:1#处理厂房照明配电箱\n2.规格:500*600*200",null,"台"]
[3,"配电箱","1.名称、型号:局部等电位端子箱",null,"台"]
[4,"配电箱","1.名称、型号:总等电位端子箱",null,"台"]
[5,"配电箱","1.名称、型号:变配电室风机配电箱",null,"台"]
[6,"配电箱","1.名称、型号:变配电室照明配电箱\n2.规格:400*500*200",null,"台"]
[7,"配电箱","1.名称、型号:处理厂房风机配电箱",null,"台"]
[8,"配电箱","1.名称、型号:处理厂房检修配电箱",null,"台"]
[9,"高压开关柜","1.名称、型号:10KV高压开关柜","1.基础型钢制作、安装\n2.本体安装、单体调试\n3.补刷（喷)油漆\n4.接地\n5.运输","台"]
[10,"低压开关柜","1.名称、型号:低压配电柜\n2.规格:1000*800*2200",null,"台"]
[11,"低压开关柜","1.名称、型号:低压配电柜\n2.规格:800*800*2200",null,"台"]
[12,"低压开关柜","1.名称、型号:风机就地操作按钮\n2.规格:300*400*200",null,"台"]
[13,"干式变压器","1.名称、型号:干式变压器",null,"台"]
[14,"高压开关柜","1.名称、型号:蒸发器高压变频器控制柜",null,"台"]
[15,"直流馈电屏","1.名称、型号:直流屏","1.本体安装\n2.基础型钢制作、安装\n3.端子板安装\n4.焊、压接线端子\n5.盘柜配线、端子接线\n6.小母线安装\n7.屏边安装\n8.补刷（喷)油漆\n9.接地","台"]
[16,"综保系统","1.名称、型号:综保系统","1.本体安装\n2.基础型钢制作、安装\n3.焊、压接线端子\n4.补刷（喷)油漆\n5.接地","台"]
[17,"槽形母线","1.名称、型号:密集型线槽","1.母线制作、安装\n2.与发电机、变压器连接\n3.与断路器、隔离开关连接\n4.刷分相漆","m"]
[18,"铺砂、盖保护板(砖）","1.名称、型号:电缆沟 800X1000","1.铺砂\n2.盖板(砖）","m"]
[19,"电缆槽盒","1.名称、型号:镀锌槽式电缆桥架 300X100","1.槽盒安装","m"]
[20,"电缆槽盒","1.名称、型号:镀锌槽式电缆桥架 300X150",null,"m"]
[21,"电缆槽盒","1.名称、型号:镀锌槽式电缆桥架 400*100",null,"m"]
[22,"电缆槽盒","1.名称、型号:镀锌槽式电缆桥架 400X150",null,"m"]
[23,"电力电缆","1.名称、型号:YJV-0.6/1KV-2*240+2*120","1.电缆敷设\n2.揭（盖）盖板","m"]
[24,"电力电缆","1.名称、型号:YJV-0.6/1KV-3*150+2*70",null,"m"]
[25,"电力电缆","1.名称、型号:YJV-0.6/1KV-3*185+2*95",null,"m"]
[26,"电力电缆","1.名称、型号:YJV-0.6/1KV-3*50",null,"m"]
[27,"电力电缆","1.名称、型号:YJV-0.6/1KV-3*70+2*35",null,"m"]
[28,"电力电缆","1.名称、型号:YJV-0.6/1KV-3*80+2*25",null,"m"]
[29,"电力电缆","1.名称、型号:YJV-0.6/1KV-3*95+2*50",null,"m"]
[30,"电力电缆","1.名称、型号:YJV-0.6/1KV-3*300",null,"m"]
[31,"电力电缆","1.名称、型号:YJV-0.6/1KV-3*95",null,"m"]
[32,"电力电缆","1.名称、型号:YJV-0.6/1KV-4*35+1*16",null,"m"]
[33,"电力电缆","1.名称、型号:YJV-0.6/1KV-4*50+1*25",null,"m"]
[34,"电力电缆","1.名称、型号:YJV-0.6/1KV-5*10",null,"m"]
[35,"电力电缆","1.名称、型号:YJV-0.6/1KV-5*16",null,"m"]
[36,"电力电缆","1.名称、型号:YJV-0.6/1KV-5*4",null,"m"]
[37,"电力电缆","1.名称、型号:YJV-0.6/1KV-5*6",null,"m"]
[38,"电力电缆","1.名称、型号:YJV-4x2.5",null,"m"]
[39,"电力电缆","1.名称、型号:YJV-4x4",null,"m"]
[null,"照明部分"]
[40,"装饰灯","1.名称、型号:A型安全出口标志灯-1X1W  36V","1.本体安装","套"]
[41,"装饰灯","1.名称、型号:A型双向疏散指示灯-1X1W  36V",null,"套"]
[42,"装饰灯","1.名称、型号:A型应急照明灯-5W  36V",null,"套"]
[43,"装饰灯","1.名称、型号:A型应急照明灯(壁装型)-5W  36V 室外IP67",null,"套"]
[44,"装饰灯","1.名称、型号:A型右向疏散指示灯-1X1W  36V",null,"套"]
[45,"装饰灯","1.名称、型号:A型左向疏散指示灯-1X1W  36V",null,"套"]
[46,"工厂灯","1.名称、型号:LED工厂灯-LED 广照型 100W 带遥控升降器",null,"套"]
[47,"装饰灯","1.名称、型号:LED投光灯-LED 防尘防水型 40W",null,"套"]
[48,"装饰灯","1.名称、型号:天棚灯-LED 18W",null,"套"]
[49,"装饰灯","1.名称、型号:自带蓄电池T8单管LED灯-LED 22W",null,"套"]
[50,"装饰灯","1.名称、型号:自带蓄电池T8双管LED灯-LED 2X22W",null,"套"]
[51,"小电器","1.名称、型号:安全型单相五孔暗装插座-86Z23-10","1.本体安装\n2.焊、压接线端子\n3.接线","个"]
[52,"小电器","1.名称、型号:空调专用插座",null,"个"]
[53,"小电器","1.名称、型号:三联开关-86K31-10",null,"个"]
[54,"小电器","1.名称、型号:双联开关-86K21-10",null,"个"]
[55,"配线","1.名称、型号:NH-BV2.5","1.配线\n2.钢索架设（拉紧装置安装）\n3.支持体（夹板、绝缘子、槽板等)安装","m"]
[56,"配线","1.名称、型号:ZR-BV4",null,"m"]
[57,"配管","1.名称、型号:PVC25","1.电线管路敷设\n2.钢索架设（拉紧装置安装）\n3.预留沟槽\n4.接地","m"]
[58,"配管","1.名称、型号:SC100",null,"m"]
[59,"配管","1.名称、型号:SC125",null,"m"]
[60,"配管","1.名称、型号:SC20",null,"m"]
[61,"配管","1.名称、型号:SC25",null,"m"]
[62,"配管","1.名称、型号:SC32",null,"m"]
[63,"配管","1.名称、型号:SC50",null,"m"]
[64,"配管","1.名称、型号:SC65",null,"m"]
[65,"配管","1.名称、型号:SC80",null,"m"]
[null,"防雷接地"]
[66,"接闪器支架","1.名称、型号:接闪器支架-Φ12热镀锌圆钢300MM","1.避雷网制作、安装\n2.跨接\n3.混凝土块制作\n4.补刷（喷)油漆","m"]
[67,"避雷引下线","1.名称、型号:防雷引下线-利用主框架柱内钢筋","1.避雷引下线制作、安装\n2.断接卡子、箱制作、安装\n3.利用主钢筋焊接\n4.补刷（喷)油漆","处"]
[68,"接地母线","1.名称、型号:桥架接地保护连接线--25X4 镀锌扁铁","1.接地母线制作、安装\n2.补刷（喷)油漆","m"]
[69,"接地母线","1.名称、型号:室外接地保护连接线--40X4不锈钢扁铁",null,"m"]
[70,"接地母线","1.名称、型号:等电位连接线--40X4",null,"m"]
[71,"避雷网","1.名称、型号:接闪带-Φ12热镀锌圆钢","1.避雷网制作、安装\n2.跨接\n3.混凝土块制作\n4.补刷（喷)油漆","m"]
[72,"接地极","1.名称、型号:接地极-Φ50镀锌钢管长2500MM","1.接地极（板、桩)制作、安装\n2.基础接地网安装\n3.补刷（喷)油漆","根"]
["报价合计",{"$nulls":13},0]

{"sheet":"1#、2#污水处理厂房-给排水","index":10,"n_rows":17,"n_cols":16,"rows_kept":17,"merged":[[0,0,0,15],[1,0,1,2],[1,4,1,7],[3,3,7,3],[8,3,12,3],[16,0,16,13]],"flags":["formulas_cached_only"]}
["工程量清单报价表"]
["工程名称：1#、2#污水处理厂房-给排水"]
["序号","项目名称","项目特征描述","工作内容","单位","工程量","人工费（元）","辅材费（元）","机械费（元）","管理费（元）","利润（元）","不含税单价（元）","税率（3%）","含税单价\n（元）","含税合价\n（元）","备注"]
[1,"螺纹阀门","1.名称、规格：减压阀 DN70","1.安装\n2.电气接线\n3.调试","个"]
[2,"螺纹阀门","1.名称、规格：截止阀 DN25",null,"个"]
[3,"螺纹阀门","1.名称、规格：闸阀 DN70",null,"个"]
[4,"螺纹阀门","1.名称、规格：倒流防止器DN25",null,"个"]
[5,"螺纹阀门","1.名称、规格：倒流防止器 DN70",null,"个"]
[6,"复合管","1.名称、规格：内涂塑钢管（内涂聚乙烯PE) DN25","1.管道安装\n2.管件安装\n3.塑料卡固定\n4.压力试验\n5.吹扫、冲洗\n6.警示带铺设","m"]
[7,"复合管","1.名称、规格：内涂塑钢管（内涂聚乙烯PE) DN32",null,"m"]
[8,"复合管","1.名称、规格：内涂塑钢管（内涂聚乙烯PE) DN40",null,"m"]
[9,"复合管","1.名称、规格：内涂塑钢管（内涂聚乙烯PE) DN50",null,"m"]
[10,"复合管","1.名称、规格：内涂塑钢管（内涂聚乙烯PE) DN70",null,"m"]
[11,"水表","1.名称、规格：水表 DN25","1.组装","组"]
[12,"套管","1.名称、规格：刚性防水套管 DN70","1.制作\n2.安装\n3.除锈、刷油","个"]
[13,"螺纹阀门","1.名称、规格：真空破坏器 DN25","1.安装\n2.电气接线\n3.调试","个"]
["报价合计",{"$nulls":13},0]

{"sheet":"办公楼-采暖","index":11,"n_rows":10,"n_cols":16,"rows_kept":10,"merged":[[0,0,0,15],[1,0,1,2],[1,4,1,7],[3,3,8,3],[9,0,9,13]],"flags":["formulas_cached_only"]}
["工程量清单报价表"]
["工程名称：办公楼-采暖"]
["序号","项目名称","项目特征描述","工作内容","单位","工程量","人工费（元）","辅材费（元）","机械费（元）","管理费（元）","利润（元）","不含税单价（元）","税率（3%）","含税单价\n（元）","含税合价\n（元）","备注"]
[1,"镀锌钢管","1.材质、规格:热镀锌钢管 DN20","1.管道安装\n2.管件制作、安装\n3.压力试验\n4.吹扫、冲洗\n5.警示带铺设","m"]
[2,"镀锌钢管","1.材质、规格:热镀锌钢管 DN25",null,"m"]
[3,"镀锌钢管","1.材质、规格:热镀锌钢管 DN32",null,"m"]
[4,"镀锌钢管","1.材质、规格:热镀锌钢管 DN40",null,"m"]
[5,"镀锌钢管","1.材质、规格:热镀锌钢管 DN50",null,"m"]
[6,"镀锌钢管","1.材质、规格:热镀锌钢管 DN65",null,"m"]
["报价合计",{"$nulls":13},0]

{"sheet":"办公楼-电气","index":12,"n_rows":57,"n_cols":16,"rows_kept":57,"merged":[[0,0,0,15],[1,0,1,2],[1,4,1,7],[4,3,8,3],[10,3,12,3],[13,3,16,3],[17,3,23,3],[24,3,26,3],[27,3,37,3],[38,3,41,3],[42,3,43,3],[44,3,46,3],[49,3,50,3],[51,3,53,3],[56,0,56,13]],"flags":["formulas_cached_only"]}
["工程量清单报价表"]
["工程名称：办公楼-电气"]
["序号","项目名称","项目特征描述","工作内容","单位","工程量","人工费（元）","辅材费（元）","机械费（元）","管理费（元）","利润（元）","不含税单价（元）","税率（3%）","含税单价\n（元）","含税合价\n（元）","备注"]
[null,"电气部分"]
[1,"配电箱","1.名称、型号:AL1001-600*800*250","1.本体安装\n2.基础型钢制作、安装\n3.焊、压接线端子\n4.补刷（喷)油漆\n5.接地","台"]
[2,"配电箱","1.名称、型号:AL2-500*600*200",null,"台"]
[3,"配电箱","1.名称、型号:AL3-500*600*200",null,"台"]
[4,"配电箱","1.名称、型号:ALE-300*500*200",null,"台"]
[5,"配电箱","1.名称、型号:HY-400*500*200",null,"台"]
[6,"配线架","1.名称、型号:光纤配线架-600*800*250","1.安装、打接","个"]
[7,"电力电缆","1.名称、型号:ZR-YJV-4*25+1*16","1.电缆敷设\n2.揭（盖）盖板","m"]
[8,"电力电缆","1.名称、型号:ZR-YJV-5*10",null,"m"]
[9,"电力电缆","1.名称、型号:ZR-YJV-5*6",null,"m"]
[10,"配线","1.名称、型号:NH-BV4","1.配线\n2.钢索架设（拉紧装置安装）\n3.支持体（夹板、绝缘子、槽板等)安装","m"]
[11,"配线","1.名称、型号:ZN-RVSP-2X2.5",null,"m"]
[12,"配线","1.名称、型号:ZR-BV2.5",null,"m"]
[13,"配线","1.名称、型号:ZR-BV4",null,"m"]
[14,"配管","1.名称、型号:PVC20","1.电线管路敷设\n2.钢索架设（拉紧装置安装）\n3.预留沟槽\n4.接地","m"]
[15,"配管","1.名称、型号:PVC25",null,"m"]
[16,"配管","1.名称、型号:SC15",null,"m"]
[17,"配管","1.名称、型号:SC20",null,"m"]
[18,"配管","1.名称、型号:SC32",null,"m"]
[19,"配管","1.名称、型号:SC40",null,"m"]
[20,"配管","1.名称、型号:SC65",null,"m"]
[21,"电缆槽盒","1.名称、型号:钢制桥架-200*200","1.槽盒安装","m"]
[22,"电缆槽盒","1.名称、型号:弱电 100*100",null,"m"]
[23,"电缆槽盒","1.名称、型号:弱电 100*50",null,"m"]
[24,"荧光灯","1.名称、型号:单管节能荧光灯-~220V 1X30W","1.本体安装","套"]
[25,"普通灯具","1.名称、型号;防水防尘吸顶灯-~220V 1X18W",null,"套"]
[26,"装饰灯","1.名称、型号:楼层标志灯-A型灯具,DC36V 1W",null,"套"]
[27,"普通灯具","1.名称、型号;墙上座灯-~220V 1X18W",null,"套"]
[28,"普通灯具","1.名称、型号;声光控开关吸顶灯-~220V 1X18W",null,"套"]
[29,"荧光灯","1.名称、型号:双管节能荧光灯-~220V 2X30W",null,"套"]
[30,"装饰灯","1.名称、型号:双向应急疏散指示标识灯-A型灯具,DC36V 1W",null,"套"]
[31,"装饰灯","1.名称、型号:应急疏散安全出口标志灯-A型灯具,DC36V 1W",null,"套"]
[32,"装饰灯","1.名称、型号:应急疏散指示标识灯-A型灯具,DC36V 1W",null,"套"]
[33,"装饰灯","1.名称、型号:应急照明灯壁装型-A型灯具,DC36V 5W",null,"套"]
[34,"装饰灯","1.名称、型号:自带蓄电池双管节能荧光灯-~220V 2X30W",null,"套"]
[35,"小电器","1.名称、型号:单联单控开关","1.本体安装\n2.焊、压接线端子\n3.接线","个"]
[36,"小电器","1.名称、型号:单联防水密闭开关",null,"个"]
[37,"小电器","1.名称、型号:电话插座-86型-RJ11",null,"个"]
[38,"小电器","1.名称、型号:二、三极安全型插座",null,"个"]
[39,"按钮","1.名称、型号：呼叫求助按钮-86型-RJ11","1.安装\n2.校接线\n3.编码\n4.调试","个"]
[40,"声光报警器","1.名称、型号：呼叫求助声光警报器-86型-RJ11",null,"个"]
[41,"小电器","1.名称、型号:三联单控开关","1.本体安装\n2.焊、压接线端子\n3.接线","个"]
[42,"小电器","1.名称、型号:双联单控开关",null,"个"]
[43,"小电器","1.名称、型号:双联防水密闭开关",null,"个"]
[44,"信息插座","1.名称、型号:信息插座-86型-RJ45","1.端接模块\n2.安装面板","个"]
[null,"防雷接地"]
[45,"配电箱","1.名称、型号:局部等电位端子箱","1.本体安装\n2.基础型钢制作、安装\n3.焊、压接线端子\n4.补刷（喷)油漆\n5.接地","台"]
[46,"配电箱","1.名称、型号:总等电位端子箱",null,"台"]
[47,"接地母线","1.名称、型号:不锈钢接地线（M）-40X4","1.接地母线制作、安装\n2.补刷（喷)油漆","m"]
[48,"接地母线","1.名称、型号:接地线(M)-镀锌扁钢  -40X4",null,"m"]
[49,"接地母线","1.名称、型号:接地线(M)-镀锌扁钢  -40X4",null,"m"]
[50,"避雷网","1.名称、型号:接闪带(M)-Φ12热镀锌圆钢","1.避雷网制作、安装\n2.跨接\n3.补刷（喷)油漆","m"]
[51,"接地极","1.名称、型号:接地极-Φ50镀锌钢管长2500MM","1.接地极（板、桩)制作、安装\n2.基础接地网安装\n3.补刷（喷)油漆","根"]
["报价合计",{"$nulls":13},0]

{"sheet":"办公楼-给排水","index":13,"n_rows":27,"n_cols":16,"rows_kept":27,"merged":[[0,0,0,15],[1,0,1,2],[1,4,1,7],[3,3,6,3],[7,3,8,3],[9,3,14,3],[15,3,18,3],[26,0,26,13]],"flags":["formulas_cached_only"]}
["工程量清单报价表"]
["工程名称：办公楼-给排水"]
["序号","项目名称","项目特征描述","工作内容","单位","工程量","人工费（元）","辅材费（元）","机械费（元）","管理费（元）","利润（元）","不含税单价（元）","税率(3%)","含税单价\n（元）","含税合价\n（元）","备注"]
[1,"螺纹阀门","1.名称、规格：闸阀 DN40","1.安装\n2.电气接线\n3.调试","个"]
[2,"螺纹阀门","1.名称、规格：闸阀 DN50",null,"个"]
[3,"螺纹阀门","1.名称、规格：止回阀 DN50",null,"个"]
[4,"螺纹阀门","1.名称、规格：自动排气阀 DN20",null,"个"]
[5,"其他成品卫生器具","1.名称、规格：地漏 DN50","1.器具安装\n2.附件安装","组"]
[6,"大便器","1.名称、规格：蹲便器",null,"组"]
[7,"复合管","1.名称、规格：内涂塑钢管（内涂聚乙烯PE) DN15","1.管道安装\n2.管件安装\n3.塑料卡固定\n4.压力试验\n5.吹扫、冲洗\n6.警示带铺设","m"]
[8,"复合管","1.名称、规格：内涂塑钢管（内涂聚乙烯PE) DN20",null,"m"]
[9,"复合管","1.名称、规格：内涂塑钢管（内涂聚乙烯PE) DN25",null,"m"]
[10,"复合管","1.名称、规格：内涂塑钢管（内涂聚乙烯PE) DN32",null,"m"]
[11,"复合管","1.名称、规格：内涂塑钢管（内涂聚乙烯PE) DN40",null,"m"]
[12,"复合管","1.名称、规格：内涂塑钢管（内涂聚乙烯PE) DN50",null,"m"]
[13,"铸铁管","1.名称、规格:柔性机制抗震铸铁管 DN100","1.管道安装\n2.管件安装\n3.压力试验\n4.吹扫、冲洗\n5.警示带铺设","m"]
[14,"铸铁管","1.名称、规格:柔性机制抗震铸铁管 DN50",null,"m"]
[15,"铸铁管","1.名称、规格:柔性机制抗震铸铁管 DN70",null,"m"]
[16,"铸铁管","1.名称、规格:柔性机制抗震铸铁管 DN80",null,"m"]
[17,"水表","1.名称、规格：水表 DN50","1.组装","组"]
[18,"洗脸盆","1.名称、规格：台式洗脸盆","1.器具安装\n2.附件安装","组"]
[19,"套管","1.名称、规格：刚性防水套管 DN50","1.制作\n2.安装\n3.除锈、刷油","个"]
[20,"洗涤盆","1.规格、类型:拖布池","1.器具安装\n2.附件安装","组"]
[21,"小便器","1.规格、类型:小便器","1.器具安装\n2.附件安装","组"]
[22,"螺纹阀门","1.名称、规格：真空破坏器 DN25","1.安装\n2.电气接线\n3.调试","个"]
[23,"大便器","1.名称、规格：坐便器","1.器具安装\n2.附件安装","组"]
["报价合计",{"$nulls":13},0]

{"sheet":"磅房-采暖","index":14,"n_rows":12,"n_cols":16,"rows_kept":12,"merged":[[0,0,0,15],[1,0,1,2],[1,4,1,7],[3,3,4,3],[5,3,8,3],[9,3,10,3],[11,0,11,13]],"flags":["formulas_cached_only"]}
["工程量清单报价表"]
["工程名称：磅房-采暖"]
["序号","项目名称","项目特征描述","工作内容","单位","工程量","人工费（元）","辅材费（元）","机械费（元）","管理费（元）","利润（元）","不含税单价（元）","税率(3%)","含税单价\n（元）","含税合价\n（元）","备注"]
[1,"镀锌钢管","1.材质、规格:热镀锌钢管 DN20","1.管道安装\n2.管件制作、安装\n3.压力试验\n4.吹扫、冲洗\n5.警示带铺设","m"]
[2,"镀锌钢管","1.材质、规格:热镀锌钢管 DN25",null,"m"]
[3,"螺纹阀门","1.材质、规格:温控阀 DN20","1.安装\n2.电气接线\n3.调试","个"]
[4,"螺纹阀门","1.材质、规格:截止阀J11T-10 DN20",null,"个"]
[5,"螺纹阀门","1.材质、规格:排气阀 DN20",null,"个"]
[6,"螺纹阀门","1.材质、规格:手动调节阀 DN25",null,"个"]
[7,"钢制散热器","1.材质、规格:钢制散热器（UR7002-600）8片","1.安装\n2.托架安装\n3.托架刷油","组"]
[8,"钢制散热器","1.材质、规格:钢制散热器（UR7002-600）18片",null,"组"]
["报价合计",{"$nulls":13},0]

{"sheet":"磅房-电气","index":15,"n_rows":23,"n_cols":16,"rows_kept":23,"merged":[[0,0,0,15],[1,0,1,2],[1,4,1,7],[5,3,6,3],[7,3,8,3],[9,3,12,3],[13,3,16,3],[19,3,20,3],[22,0,22,13]],"flags":["formulas_cached_only"]}
["工程量清单报价表"]
["工程名称：磅房-电气"]
["序号","项目名称","项目特征描述","工作内容","单位","工程量","人工费（元）","辅材费（元）","机械费（元）","管理费（元）","利润（元）","不含税单价（元）","税率（3%）","含税单价\n（元）","含税合价\n（元）","备注"]
[null,"电气部分"]
[1,"配电箱","1.名称、型号:AL101-600*500*100","1.本体安装\n2.基础型钢制作、安装\n3.焊、压接线端子\n4.补刷（喷)油漆\n5.接地","台"]
[2,"配线","1.名称、型号:ZR-BV2.5","1.配线\n2.钢索架设（拉紧装置安装）\n3.支持体（夹板、绝缘子、槽板等)安装","m"]
[3,"配线","1.名称、型号:ZR-BV4",null,"m"]
[4,"配管","1.名称、型号:PVC20","1.电线管路敷设\n2.钢索架设（拉紧装置安装）\n3.预留沟槽\n4.接地","m"]
[5,"配管","1.名称、型号:PVC25",null,"m"]
[6,"普通灯具","1.名称、型号;防水防尘吸顶灯-~220V 1X18W","1.本体安装","套"]
[7,"普通灯具","1.名称、型号;室外雨棚灯-LED 18W  IP67",null,"套"]
[8,"荧光灯","1.名称、型号:双管节能荧光灯-220V 36W",null,"套"]
[9,"普通灯具","1.名称、型号;一体化太阳能灯-LED 1X12W",null,"套"]
[10,"小电器","1.名称、型号:单联防水密闭开关","1.本体安装\n2.焊、压接线端子\n3.接线","个"]
[11,"小电器","1.名称、型号:二、三极安全型插座",null,"个"]
[12,"小电器","1.名称、型号:三联单控开关",null,"个"]
[13,"小电器","1.名称、型号:双联单控开关",null,"个"]
[null,"防雷接地"]
[14,"配电箱","1.名称、型号:总等电位端子箱","1.本体安装\n2.基础型钢制作、安装\n3.焊、压接线端子\n4.补刷（喷)油漆\n5.接地","台"]
[15,"接地母线","1.名称、型号:不锈钢接地线（M）-40X4","1.接地母线制作、安装\n2.补刷（喷)油漆","m"]
[16,"接地母线","1.名称、型号:接地线(M)-镀锌扁钢  -40X4",null,"m"]
[17,"接地极","1.名称、型号:接地极-Φ50镀锌钢管长2500MM","1.接地极（板、桩)制作、安装\n2.基础接地网安装\n3.补刷（喷)油漆","根"]
["报价合计",{"$nulls":13},0]

{"sheet":"磅房-给排水","index":16,"n_rows":23,"n_cols":16,"rows_kept":23,"merged":[[0,0,0,15],[1,0,1,2],[1,4,1,7],[4,3,6,3],[9,3,11,3],[13,3,15,3],[16,3,17,3],[20,3,21,3],[22,0,22,13]],"flags":["formulas_cached_only"]}
["工程量清单报价表"]
["工程名称：磅房-给排水"]
["序号","项目名称","项目特征描述","工作内容","单位","工程量","人工费（元）","辅材费（元）","机械费（元）","管理费（元）","利润（元）","不含税单价（元）","税率(3%)","含税单价\n（元）","含税合价\n（元）","备注"]
[1,"塑料管","1.材质、规格:金属软管≥400mm","1.管道安装\n2.管件安装\n3.塑料卡固定\n4.阻火圈安装\n5.压力试验\n6.吹扫、冲洗\n7.警示带铺设","m"]
[2,"螺纹阀门","1.名称、规格：截止阀 DN25","1.安装\n2.电气接线\n3.调试","个"]
[3,"螺纹阀门","1.名称、规格：闸阀 DN25",null,"个"]
[4,"螺纹阀门","1.名称、规格：止回阀 DN25",null,"个"]
[5,"其他成品卫生器具","1.名称、规格：地漏 DN50","1.器具安装\n2.附件安装","组"]
[6,"热水器、开水炉","1.名称、规格：电热水器","1.安装\n2.附件安装","台"]
[7,"复合管","1.名称、规格：内涂塑钢管（内涂聚乙烯PE) DN15","1.管道安装\n2.管件安装\n3.塑料卡固定\n4.压力试验\n5.吹扫、冲洗\n6.警示带铺设","m"]
[8,"复合管","1.名称、规格：内涂塑钢管（内涂聚乙烯PE) DN20",null,"m"]
[9,"复合管","1.名称、规格：内涂塑钢管（内涂聚乙烯PE) DN25",null,"m"]
[10,"淋浴器","1.名称、规格：淋浴器","1.器具安装\n2.附件安装","套"]
[11,"铸铁管","1.名称、规格:柔性机制抗震铸铁管 DN100","1.管道安装\n2.管件安装\n3.压力试验\n4.吹扫、冲洗\n5.警示带铺设","m"]
[12,"铸铁管","1.名称、规格:柔性机制抗震铸铁管 DN50",null,"m"]
[13,"铸铁管","1.名称、规格:柔性机制抗震铸铁管 DN70",null,"m"]
[14,"塑料管","1.材质、规格:热水DN15","1.管道安装\n2.管件安装\n3.塑料卡固定\n4.阻火圈安装\n5.压力试验\n6.吹扫、冲洗\n7.警示带铺设","m"]
[15,"塑料管","1.材质、规格:热水DN20",null,"m"]
[16,"水表","1.名称、规格：水表 DN25","1.组装","组"]
[17,"套管","1.名称、规格：刚性防水套管 DN25","1.制作\n2.安装\n3.除锈、刷油","个"]
[18,"洗脸盆","1.名称、规格：台式洗脸盆","1.器具安装\n2.附件安装","组"]
[19,"大便器","1.名称、规格：坐便器",null,"组"]
["报价合计",{"$nulls":13},0]

{"sheet":"库房-电气","index":17,"n_rows":23,"n_cols":16,"rows_kept":23,"merged":[[0,0,0,15],[1,0,1,2],[1,4,1,7],[4,3,5,3],[6,3,7,3],[8,3,9,3],[10,3,11,3],[12,3,16,3],[19,3,20,3],[22,0,22,13]],"flags":["formulas_cached_only"]}
["工程量清单报价表"]
["工程名称：库房-电气"]
["序号","项目名称","项目特征描述","工作内容","单位","工程量","人工费（元）","辅材费（元）","机械费（元）","管理费（元）","利润（元）","不含税单价（元）","税率（3%）","含税单价\n（元）","含税合价\n（元）","备注"]
[null,"电气"]
[1,"配电箱","1.名称、型号:AL201-600*500*100","1.本体安装\n2.基础型钢制作、安装\n3.焊、压接线端子\n4.补刷（喷)油漆\n5.接地","台"]
[2,"配电箱","1.名称、型号:AP801-500*600*200",null,"台"]
[3,"配线","1.名称、型号:ZR-BV2.5","1.配线\n2.钢索架设（拉紧装置安装）\n3.支持体（夹板、绝缘子、槽板等)安装","m"]
[4,"配线","1.名称、型号:ZR-BV4",null,"m"]
[5,"配管","1.名称、型号:PVC20","1.电线管路敷设\n2.钢索架设（拉紧装置安装）\n3.预留沟槽\n4.接地","m"]
[6,"配管","1.名称、型号:PVC25",null,"m"]
[7,"装饰灯","1.名称、型号:单管节能荧光灯-~220V 2X30W","1.本体安装","套"]
[8,"普通灯具","1.名称、型号:吸顶灯-~220V 1X18W",null,"套"]
[9,"小电器","1.名称、型号:单联单控开关","1.本体安装\n2.焊、压接线端子\n3.接线","个"]
[10,"小电器","1.名称、型号:二、三极安全型插座",null,"个"]
[11,"小电器","1.名称、型号:风机盘管温控开关",null,"个"]
[12,"小电器","1.名称、型号:双联单控开关",null,"个"]
[13,"小电器","1.名称、型号:四联单控开关",null,"个"]
[null,"防雷接地"]
[14,"配电箱","1.名称、型号:总等电位端子箱（台）-TD28","1.本体安装\n2.基础型钢制作、安装\n3.焊、压接线端子\n4.补刷（喷)油漆\n5.接地","台"]
[15,"接地母线","1.名称、型号:不锈钢接地线（M）-40X4","1.接地母线制作、安装\n2.补刷（喷)油漆","m"]
[16,"接地母线","1.名称、型号:镀锌扁钢接地线（M)--40X4",null,"m"]
[17,"接地极","1.名称、型号:镀锌钢管接地极（根）-SC50  L=2.5米","1.接地极（板、桩)制作、安装\n2.基础接地网安装\n3.补刷（喷)油漆","根"]
["报价合计",{"$nulls":13},0]

{"sheet":"库房-给排水","index":18,"n_rows":16,"n_cols":16,"rows_kept":16,"merged":[[0,0,0,15],[1,0,1,2],[1,4,1,7],[3,3,5,3],[7,3,9,3],[12,3,13,3],[15,0,15,13]],"flags":["formulas_cached_only"]}
["工程量清单报价表"]
["工程名称：库房-给排水"]
["序号","项目名称","项目特征描述","工作内容","单位","工程量","人工费（元）","辅材费（元）","机械费（元）","管理费（元）","利润（元）","不含税单价（元）","税率（3%）","含税单价\n（元）","含税合价\n（元）","备注"]
[1,"螺纹阀门","1.名称、规格：减压阀 DN40","1.安装\n2.电气接线\n3.调试","个"]
[2,"螺纹阀门","1.名称、规格：截止阀 DN25",null,"个"]
[3,"螺纹阀门","1.名称、规格：闸阀 DN40",null,"个"]
[4,"其他成品卫生器具","1.名称、规格：地漏 DN150","1.器具安装\n2.附件安装","组"]
[5,"复合管","1.名称、规格：内涂塑钢管（内涂聚乙烯PE) DN25","1.管道安装\n2.管件安装\n3.塑料卡固定\n4.压力试验\n5.吹扫、冲洗\n6.警示带铺设","m"]
[6,"复合管","1.名称、规格：内涂塑钢管（内涂聚乙烯PE) DN32",null,"m"]
[7,"复合管","1.名称、规格：内涂塑钢管（内涂聚乙烯PE) DN40",null,"m"]
[8,"铸铁管","1.名称、规格:柔性机制抗震铸铁管 DN150","1.管道安装\n2.管件安装\n3.压力试验\n4.吹扫、冲洗\n5.警示带铺设","m"]
[9,"水表","1.名称、规格：水表 DN25","1.组装","组"]
[10,"套管","1.名称、规格：刚性防水套管 DN40","1.制作\n2.安装\n3.除锈、刷油","个"]
[11,"套管","1.名称、规格：刚性防水套管 DN150",null,"个"]
[12,"螺纹阀门","1.名称、规格：真空破坏器 DN25","1.安装\n2.电气接线\n3.调试","个"]
["报价合计",{"$nulls":13},0]

{"sheet":"门卫-采暖","index":19,"n_rows":9,"n_cols":16,"rows_kept":9,"merged":[[0,0,0,15],[1,0,1,2],[1,4,1,7],[3,3,7,3],[8,0,8,13]],"flags":["formulas_cached_only"]}
["工程量清单报价表"]
["工程名称：门卫-采暖"]
["序号","项目名称","项目特征描述","工作内容","单位","工程量","人工费（元）","辅材费（元）","机械费（元）","管理费（元）","利润（元）","不含税单价（元）","税率（3%）","含税单价\n（元）","含税合价\n（元）","备注"]
[1,"镀锌钢管","1.材质、规格:热镀锌钢管 DN20","1.管道安装\n2.管件制作、安装\n3.压力试验\n4.吹扫、冲洗\n5.警示带铺设","m"]
[2,"镀锌钢管","1.材质、规格:热镀锌钢管 DN25",null,"m"]
[3,"镀锌钢管","1.材质、规格:热镀锌钢管 DN32",null,"m"]
[4,"镀锌钢管","1.材质、规格:热镀锌钢管 DN40",null,"m"]
[5,"镀锌钢管","1.材质、规格:热镀锌钢管 DN50",null,"m"]
["报价合计",{"$nulls":13},0]

{"sheet":"门卫-电气","index":20,"n_rows":22,"n_cols":16,"rows_kept":22,"merged":[[0,0,0,15],[1,0,1,2],[1,4,1,7],[5,3,6,3],[7,3,8,3],[9,3,12,3],[13,3,16,3],[21,0,21,13]],"flags":["formulas_cached_only"]}
["工程量清单报价表"]
["工程名称：门卫-电气"]
["序号","项目名称","项目特征描述","工作内容","单位","工程量","人工费（元）","辅材费（元）","机械费（元）","管理费（元）","利润（元）","不含税单价（元）","税率（3%）","含税单价\n（元）","含税合价\n（元）","备注"]
[null,"电气部分"]
[1,"配电箱","1.名称、型号:AL1401-500*700*200","1.本体安装\n2.基础型钢制作、安装\n3.焊、压接线端子\n4.补刷（喷)油漆\n5.接地","台"]
[2,"配线","1.名称、型号:ZR-BV2.5","1.配线\n2.钢索架设（拉紧装置安装）\n3.支持体（夹板、绝缘子、槽板等)安装","m"]
[3,"配线","1.名称、型号:ZR-BV4",null,"m"]
[4,"配管","1.名称、型号:PVC20","1.电线管路敷设\n2.钢索架设（拉紧装置安装）\n3.预留沟槽\n4.接地","m"]
[5,"配管","1.名称、型号:PVC25",null,"m"]
[6,"荧光灯","1.名称、型号:单管LED灯-LEDT8 30W","1.本体安装","套"]
[7,"普通灯具","1.名称、型号;防水防尘吸顶灯-~220V 1X18W",null,"套"]
[8,"普通灯具","1.名称、型号;室外雨棚灯-LED 18W  IP67",null,"套"]
[9,"荧光灯","1.名称、型号:双管节能荧光灯-~220V 2X30W",null,"套"]
[10,"小电器","1.名称、型号:单联单控开关","1.本体安装\n2.焊、压接线端子\n3.接线","个"]
[11,"小电器","1.名称、型号:二、三极安全型插座",null,"个"]
[12,"小电器","1.名称、型号:空调插座",null,"个"]
[13,"小电器","1.名称、型号:双联单控开关",null,"个"]
[null,"防雷接地"]
[14,"配电箱","1.名称、型号:总等电位端子箱","1.本体安装\n2.基础型钢制作、安装\n3.焊、压接线端子\n4.补刷（喷)油漆\n5.接地","台"]
[15,"接地母线","1.名称、型号:镀锌扁钢接地线（M)-10","1.接地母线制作、安装\n2.补刷（喷)油漆","m"]
[16,"接地极","1.名称、型号:接地极-Φ50镀锌钢管长2500MM","1.接地极（板、桩)制作、安装\n2.基础接地网安装\n3.补刷（喷)油漆","根"]
["报价合计",{"$nulls":13},0]

{"sheet":"门卫-给排水","index":21,"n_rows":22,"n_cols":16,"rows_kept":22,"merged":[[0,0,0,15],[1,0,1,2],[1,4,1,7],[4,3,6,3],[9,3,11,3],[13,3,14,3],[15,3,16,3],[19,3,20,3],[21,0,21,13]],"flags":["formulas_cached_only"]}
["工程量清单报价表"]
["工程名称：门卫-给排水"]
["序号","项目名称","项目特征描述","工作内容","单位","工程量","人工费（元）","辅材费（元）","机械费（元）","管理费（元）","利润（元）","不含税单价（元）","税率（3%）","含税单价\n（元）","含税合价\n（元）","备注"]
[1,"塑料管","1.材质、规格:金属软管≥400mm","1.管道安装\n2.管件安装\n3.塑料卡固定\n4.阻火圈安装\n5.压力试验\n6.吹扫、冲洗\n7.警示带铺设","m"]
[2,"螺纹阀门","1.名称、规格：截止阀 DN25","1.安装\n2.电气接线\n3.调试","个"]
[3,"螺纹阀门","1.名称、规格：闸阀 DN25",null,"个"]
[4,"螺纹阀门","1.名称、规格：止回阀 DN25",null,"个"]
[5,"其他成品卫生器具","1.名称、规格：地漏 DN50","1.器具安装\n2.附件安装","组"]
[6,"热水器、开水炉","1.名称、规格：电热水器","1.安装\n2.附件安装","台"]
[7,"复合管","1.名称、规格：内涂塑钢管（内涂聚乙烯PE) DN15","1.管道安装\n2.管件安装\n3.塑料卡固定\n4.压力试验\n5.吹扫、冲洗\n6.警示带铺设","m"]
[8,"复合管","1.名称、规格：内涂塑钢管（内涂聚乙烯PE) DN20",null,"m"]
[9,"复合管","1.名称、规格：内涂塑钢管（内涂聚乙烯PE) DN25",null,"m"]
[10,"淋浴器","1.名称、规格：淋浴器","1.器具安装\n2.附件安装","套"]
[11,"铸铁管","1.名称、规格:柔性机制抗震铸铁管 DN100","1.管道安装\n2.管件安装\n3.压力试验\n4.吹扫、冲洗\n5.警示带铺设","m"]
[12,"铸铁管","1.名称、规格:柔性机制抗震铸铁管 DN50",null,"m"]
[13,"塑料管","1.材质、规格:热水DN15","1.管道安装\n2.管件安装\n3.塑料卡固定\n4.阻火圈安装\n5.压力试验\n6.吹扫、冲洗\n7.警示带铺设","m"]
[14,"塑料管","1.材质、规格:热水DN20",null,"m"]
[15,"水表","1.名称、规格：水表 DN25","1.组装","组"]
[16,"套管","1.名称、规格：刚性防水套管 DN25","1.制作\n2.安装\n3.除锈、刷油","个"]
[17,"洗脸盆","1.名称、规格：台式洗脸盆","1.器具安装\n2.附件安装","组"]
[18,"大便器","1.名称、规格：坐便器",null,"组"]
["报价合计",{"$nulls":13},0]

{"sheet":"热泵间-采暖","index":22,"n_rows":28,"n_cols":16,"rows_kept":28,"merged":[[0,0,0,15],[1,0,1,2],[1,4,1,7],[3,3,6,3],[7,3,16,3],[27,0,27,13]],"flags":["formulas_cached_only"]}
["工程量清单报价表"]
["工程名称：热泵间-采暖"]
["序号","项目名称","项目特征描述","工作内容","单位","工程量","人工费（元）","辅材费（元）","机械费（元）","管理费（元）","利润（元）","不含税单价（元）","税率（3%）","含税单价\n（元）","含税合价\n（元）","备注"]
[1,"镀锌钢管","1.材质、规格:热镀锌钢管 DN20","1.管道安装\n2.管件制作、安装\n3.压力试验\n4.吹扫、冲洗\n5.警示带铺设","m"]
[2,"镀锌钢管","1.材质、规格:热镀锌钢管 DN25",null,"m"]
[3,"镀锌钢管","1.材质、规格:热镀锌钢管 DN32",null,"m"]
[4,"镀锌钢管","1.材质、规格:无缝钢管 DN150",null,"m"]
[5,"螺纹阀门","1.材质、规格:温控阀 DN20","1.安装\n2.电气接线\n3.调试","个"]
[6,"螺纹阀门","1.材质、规格:截止阀J11T-10 DN20",null,"个"]
[7,"螺纹阀门","1.材质、规格:安全阀 DN15  Pn=1.6MPa",null,"个"]
[8,"焊接法兰阀门","1.材质、规格:安全阀 DN150  Pn=1.6MPa",null,"个"]
[9,"螺纹阀门","1.材质、规格:排气阀 DN20",null,"个"]
[10,"螺纹阀门","1.材质、规格:手动调节阀 DN32",null,"个"]
[11,"焊接法兰阀门","1.材质、规格:硬密封蝶阀 D343H-16C DN150",null,"个"]
[12,"螺纹阀门","1.材质、规格:闸阀   Z41H-16C DN25",null,"个"]
[13,"焊接法兰阀门","1.材质、规格:闸阀   Z41H-16C DN65",null,"个"]
[14,"焊接法兰阀门","1.材质、规格:闸阀   Z41H-16C DN150",null,"个"]
[15,"循环水泵","1.材质、规格:补水泵G=2m3/h ,H=20m N=0.37KW","1.本体安装\n2.附件安装\n3.电动机安装\n4.设备表面底漆修补","台"]
[16,"除污器(过滤器）","1.材质、规格:除污器 DN150 Pn=1.0MPa","1.安装","组"]
[17,"钢制散热器","1.材质、规格:钢制散热器（UR7002-600）12片","1.安装\n2.托架安装\n3.托架刷油","组"]
[18,"循环水泵","1.材质、规格:螺杆式超低温空气源热泵","1.本体安装\n2.附件安装\n3.电动机安装\n4.设备表面底漆修补","台"]
[19,"热计量装置","1.材质、规格:热计量装置","1.设备安装\n2.附件安装\n3.调试\n4.减震装置制作、安装","套"]
[20,"压力仪表","1.名称、规格：压力表","1.本体安装\n2.压力表弯制作、安装\n3.挠性管安装\n4.取源部件配合安装\n5.单体校验调整\n6.脱脂\n7.支架制作、安装","台"]
[21,"热力入口装置","1.名称、规格：热力入口装置","1.本体安装\n2.附件安装\n3调试","套"]
[22,"软化水处理装置","1.名称：软化水处理装置\n2.规格：流量：1m3/h  电功率：1KW","1.本体安装\n2.附件安装\n3.调试","个"]
[23,"水箱","1.名称：软化水箱\n2.规格：有效容积1mm3","1.制作\n2.安装","台"]
[24,"循环水泵","1.名称：系统循环泵\n2.规格：G=50m3/h H=35m N=15kW","1.本体安装\n2.附件安装\n3.电动机安装\n4.设备表面底漆修补","台"]
["报价合计",{"$nulls":13},0]

{"sheet":"热泵间-电气","index":23,"n_rows":32,"n_cols":16,"rows_kept":32,"merged":[[0,0,0,15],[1,0,1,2],[1,4,1,7],[4,3,10,3],[11,3,14,3],[15,3,19,3],[20,3,22,3],[23,3,25,3],[28,3,30,3],[31,0,31,13]],"flags":["formulas_cached_only"]}
["工程量清单报价表"]
["工程名称：热泵间-电气"]
["序号","项目名称","项目特征描述","工作内容","单位","工程量","人工费（元）","辅材费（元）","机械费（元）","管理费（元）","利润（元）","不含税单价（元）","税率（3%）","含税单价\n（元）","含税合价\n（元）","备注"]
[null,"电气"]
[1,"配电箱","1.名称、型号:AL1301-450*600*180","1.本体安装\n2.基础型钢制作、安装\n3.焊、压接线端子\n4.补刷（喷)油漆\n5.接地","台"]
[2,"配电箱","1.名称、型号:AP1301-450*600*250",null,"台"]
[3,"配电箱","1.名称、型号:AP1302-450*600*250",null,"台"]
[4,"配电箱","1.名称、型号:AP1303-450*600*250",null,"台"]
[5,"配电箱","1.名称、型号:AP1304-450*600*250",null,"台"]
[6,"配电箱","1.名称、型号:AP1305-450*600*250",null,"台"]
[7,"配电箱","1.名称、型号:AP1306-450*600*250",null,"台"]
[8,"配线","1.名称、型号:ZR-BV10","1.配线\n2.钢索架设（拉紧装置安装）\n3.支持体（夹板、绝缘子、槽板等)安装","m"]
[9,"配线","1.名称、型号:ZR-BV16",null,"m"]
[10,"配线","1.名称、型号:ZR-BV2.5",null,"m"]
[11,"配线","1.名称、型号:ZR-BV4",null,"m"]
[12,"配管","1.名称、型号:PVC20","1.电线管路敷设\n2.钢索架设（拉紧装置安装）\n3.预留沟槽\n4.接地","m"]
[13,"配管","1.名称、型号:PVC25",null,"m"]
[14,"配管","1.名称、型号:SC20",null,"m"]
[15,"配管","1.名称、型号:SC40",null,"m"]
[16,"配管","1.名称、型号:SC50",null,"m"]
[17,"普通灯具","1.名称、型号;防水防尘吸顶灯-~220V 1X30W","1.本体安装","套"]
[18,"普通灯具","1.名称、型号:吸顶灯-~220V 1X18W",null,"套"]
[19,"装饰灯","1.名称、型号:自带蓄电池双管节能荧光灯-~220V 2X30W",null,"套"]
[20,"小电器","1.名称、型号:二、三极安全型插座","1.本体安装\n2.焊、压接线端子\n3.接线","个"]
[21,"小电器","1.名称、型号:三联防水密闭开关",null,"个"]
[22,"小电器","1.名称、型号:四联单控开关",null,"个"]
[null,"设备"]
[23,"配电箱","1.名称、型号:AC-软化水处理装置控制箱","1.本体安装\n2.基础型钢制作、安装\n3.焊、压接线端子\n4.补刷（喷)油漆\n5.接地","台"]
[24,"循环水泵","1.名称、型号:补水泵","1.本体安装\n2.附件安装\n3.电动机安装\n4.设备表面底漆修补","台"]
[25,"循环水泵","1.名称、型号:热泵循环泵",null,"台"]
[26,"循环水泵","1.名称、型号:循环泵",null,"台"]
["报价合计",{"$nulls":13},0]

{"sheet":"热泵间-给排水","index":24,"n_rows":17,"n_cols":16,"rows_kept":17,"merged":[[0,0,0,15],[1,0,1,2],[1,4,1,7],[3,3,8,3],[16,0,16,13]],"flags":["formulas_cached_only"]}
["工程量清单报价表"]
["工程名称：热泵间-给排水"]
["序号","项目名称","项目特征描述","工作内容","单位","工程量","人工费（元）","辅材费（元）","机械费（元）","管理费（元）","利润（元）","不含税单价（元）","税率(3%)","含税单价\n（元）","含税合价\n（元）","备注"]
[1,"螺纹阀门","1.名称、规格：电磁阀 DN50","1.安装\n2.电气接线\n3.调试","个"]
[2,"螺纹阀门","1.名称、规格：消音止回阀 DN50",null,"个"]
[3,"螺纹阀门","1.名称、规格：闸阀 DN50",null,"个"]
[4,"焊接法兰阀门","1.名称、规格：闸阀 DN100",null,"个"]
[5,"螺纹阀门","1.名称、规格：止回阀 DN50",null,"个"]
[6,"螺纹阀门","1.名称、规格：Y型除污器 DN50",null,"个"]
[7,"其他成品卫生器具","1.名称、规格：地漏 DN100","1.器具安装\n2.附件安装","组"]
[8,"螺纹阀门","1.名称、规格：可曲挠橡胶头 DN50","1.安装\n2.电气接线\n3.调试","个"]
[9,"铸铁管","1.名称、规格:柔性机制抗震铸铁管 DN100","1.管道安装\n2.管件安装\n3.压力试验\n4.吹扫、冲洗\n5.警示带铺设","m"]
[10,"水表","1.名称、规格：水表 DN50","1.组装","组"]
[11,"套管","1.名称、规格：刚性防水套管 DN50","1.制作\n2.安装\n3.除锈、刷油","个"]
[12,"压力仪表","1.名称、规格：压力表","1.本体安装\n2.压力表弯制作、安装\n3.挠性管安装\n4.取源部件配合安装\n5.单体校验调整\n6.脱脂\n7.支架制作、安装","台"]
[13,"复合管","1.名称、规格：内涂塑钢管（内涂聚乙烯PE) DN50","1.管道安装\n2.管件安装\n3.塑料卡固定\n4.压力试验\n5.吹扫、冲洗\n6.警示带铺设","m"]
["报价合计",{"$nulls":13},0]

{"sheet":"修理车间-采暖","index":25,"n_rows":17,"n_cols":16,"rows_kept":17,"merged":[[0,0,0,15],[1,0,1,2],[1,4,1,7],[3,3,6,3],[7,3,10,3],[11,3,15,3],[16,0,16,13]],"flags":["formulas_cached_only"]}
["工程量清单报价表"]
["工程名称：修理车间-采暖"]
["序号","项目名称","项目特征描述","工作内容","单位","工程量","人工费（元）","辅材费（元）","机械费（元）","管理费（元）","利润（元）","不含税单价（元）","税率（3%）","含税单价\n（元）","含税合价\n（元）","备注"]
[1,"镀锌钢管","1.材质、规格:热镀锌钢管 DN25","1.管道安装\n2.管件制作、安装\n3.压力试验\n4.吹扫、冲洗\n5.警示带铺设","m"]
[2,"镀锌钢管","1.材质、规格:热镀锌钢管 DN32",null,"m"]
[3,"镀锌钢管","1.材质、规格:热镀锌钢管 DN40",null,"m"]
[4,"镀锌钢管","1.材质、规格:热镀锌钢管 DN50",null,"m"]
[5,"螺纹阀门","1.材质、规格:温控阀 DN20","1.安装\n2.电气接线\n3.调试","个"]
[6,"螺纹阀门","1.材质、规格:截止阀J11T-10 DN20",null,"个"]
[7,"螺纹阀门","1.材质、规格:排气阀 DN20",null,"个"]
[8,"螺纹阀门","1.材质、规格:手动调节阀 DN50",null,"个"]
[9,"钢制散热器","1.材质、规格:钢制散热器（UR7002-600）8片","1.安装\n2.托架安装\n3.托架刷油","组"]
[10,"钢制散热器","1.材质、规格:钢制散热器（UR7002-600）12片",null,"组"]
[11,"钢制散热器","1.材质、规格:钢制散热器（UR7002-600）16片",null,"组"]
[12,"钢制散热器","1.材质、规格:钢制散热器（UR7002-600）20片",null,"组"]
[13,"钢制散热器","1.材质、规格:钢制散热器（UR7002-600）24片",null,"组"]
["报价合计",{"$nulls":13},0]

{"sheet":"修理车间-电气","index":26,"n_rows":41,"n_cols":16,"rows_kept":41,"merged":[[0,0,0,15],[1,0,1,2],[1,4,1,7],[4,3,10,3],[11,3,13,3],[14,3,20,3],[23,3,26,3],[28,3,33,3],[35,3,36,3],[37,3,38,3],[40,0,40,13]],"flags":["formulas_cached_only"]}
["工程量清单报价表"]
["工程名称：修理车间-电气"]
["序号","项目名称","项目特征描述","工作内容","单位","工程量","人工费（元）","辅材费（元）","机械费（元）","管理费（元）","利润（元）","不含税单价（元）","税率（3%）","含税单价\n（元）","含税合价\n（元）","备注"]
[null,"电气部分"]
[1,"配电箱","1.名称、型号:AL901-450*600*180","1.本体安装\n2.基础型钢制作、安装\n3.焊、压接线端子\n4.补刷（喷)油漆\n5.接地","台"]
[2,"配电箱","1.名称、型号:AP901-450*600*250",null,"台"]
[3,"配电箱","1.名称、型号:FJX901-450*500*250",null,"台"]
[4,"配电箱","1.名称、型号:JXX901-450*200*250",null,"台"]
[5,"配电箱","1.名称、型号:JXX902-450*200*250",null,"台"]
[6,"配电箱","1.名称、型号:JXX903-450*200*250",null,"台"]
[7,"配电箱","1.名称、型号:电动卷帘门控制箱-450*200*180",null,"台"]
[8,"电力电缆","1.名称、型号:ZR-YJV-4*2.5","1.电缆敷设\n2.揭（盖）盖板","m"]
[9,"电力电缆","1.名称、型号:ZR-YJV-5*10",null,"m"]
[10,"电力电缆","1.名称、型号:ZR-YJV-5*16",null,"m"]
[11,"配线","1.名称、型号:ZR-BV2.5","1.配线\n2.钢索架设（拉紧装置安装）\n3.支持体（夹板、绝缘子、槽板等)安装","m"]
[12,"配线","1.名称、型号:ZR-BV4",null,"m"]
[13,"配管","1.名称、型号:PVC20",null,"m"]
[14,"配管","1.名称、型号:PVC25",null,"m"]
[15,"配管","1.名称、型号:SC25",null,"m"]
[16,"配管","1.名称、型号:SC40",null,"m"]
[17,"配管","1.名称、型号:SC50",null,"m"]
[18,"普通灯具","1.名称、型号;LED工矿灯-~220V 1X100W","1.本体安装","套"]
[19,"多功能媒体箱","1.名称、型号;多功能媒体箱-220V 36W","1.本体安装\n2.接线","台"]
[20,"普通灯具","1.名称、型号;防水防尘吸顶灯-~220V 1X18W","1.本体安装","套"]
[21,"普通灯具","1.名称、型号;声光控开关吸顶灯-~220V 1X18W",null,"套"]
[22,"荧光灯","1.名称、型号:双管节能荧光灯-~220V 2X30W",null,"套"]
[23,"普通灯具","1.名称、型号;吸顶灯-~220V 1X18W",null,"套"]
[24,"信息插座","1.名称、型号:信息插座-86型-RJ45","1.端接模块\n2.安装面板","个"]
[25,"小电器","1.名称、型号:单联单控开关","1.本体安装\n2.焊、压接线端子\n3.接线","个"]
[26,"小电器","1.名称、型号:电热水器插座",null,"个"]
[27,"小电器","1.名称、型号:二、三极安全型插座",null,"个"]
[28,"小电器","1.名称、型号:双联单控开关",null,"个"]
[29,"小电器","1.名称、型号:三联单控开关",null,"个"]
[30,"小电器","1.名称、型号:四联单控开关",null,"个"]
[null,"防雷接地"]
[31,"配电箱","1.名称、型号:总等电位端子箱局部等电位端子箱(台）-TD28","1.本体安装\n2.基础型钢制作、安装\n3.焊、压接线端子\n4.补刷（喷)油漆\n5.接地","台"]
[32,"配电箱","1.名称、型号:总等电位端子箱(台）-TD28",null,"台"]
[33,"接地母线","1.名称、型号:不锈钢接地线(M）--40X4","1.接地母线制作、安装\n2.补刷（喷)油漆","m"]
[34,"接地母线","1.名称、型号:镀锌扁钢接地线(M）--40X4",null,"m"]
[35,"接地极","1.名称、型号:镀锌钢管接地极(根）-SC50  L=2.5米","1.接地极（板、桩)制作、安装\n2.基础接地网安装\n3.补刷（喷)油漆","根"]
["报价合计",{"$nulls":13},0]

{"sheet":"修理车间-给排水","index":27,"n_rows":23,"n_cols":16,"rows_kept":23,"merged":[[0,0,0,15],[1,0,1,2],[1,4,1,7],[4,3,6,3],[9,3,12,3],[14,3,15,3],[17,3,18,3],[20,3,21,3],[22,0,22,13]],"flags":["formulas_cached_only"]}
["工程量清单报价表"]
["工程名称：修理车间-给排水"]
["序号","项目名称","项目特征描述","工作内容","单位","工程量","人工费（元）","辅材费（元）","机械费（元）","管理费（元）","利润（元）","不含税单价（元）","税率（3%）","含税单价\n（元）","含税合价\n（元）","备注"]
[1,"塑料管","1.材质、规格:金属软管≥400mm","1.管道安装\n2.管件安装\n3.塑料卡固定\n4.阻火圈安装\n5.压力试验\n6.吹扫、冲洗\n7.警示带铺设","m"]
[2,"螺纹阀门","1.名称、规格：截止阀 DN25","1.安装\n2.电气接线\n3.调试","个"]
[3,"螺纹阀门","1.名称、规格：闸阀 DN32",null,"个"]
[4,"螺纹阀门","1.名称、规格：自动排气阀 DN20",null,"个"]
[5,"其他成品卫生器具","1.名称、规格：地漏 DN50","1.器具安装\n2.附件安装","组"]
[6,"热水器、开水炉","1.名称、规格：电热水器","1.安装\n2.附件安装","台"]
[7,"复合管","1.名称、规格：内涂塑钢管（内涂聚乙烯PE) DN15","1.管道安装\n2.管件安装\n3.塑料卡固定\n4.压力试验\n5.吹扫、冲洗\n6.警示带铺设","m"]
[8,"复合管","1.名称、规格：内涂塑钢管（内涂聚乙烯PE) DN20",null,"m"]
[9,"复合管","1.名称、规格：内涂塑钢管（内涂聚乙烯PE) DN25",null,"m"]
[10,"复合管","1.名称、规格：内涂塑钢管（内涂聚乙烯PE) DN32",null,"m"]
[11,"淋浴器","1.名称、规格：淋浴器","1.器具安装\n2.附件安装","套"]
[12,"铸铁管","1.名称、规格:柔性机制抗震铸铁管 DN100","1.管道安装\n2.管件安装\n3.压力试验\n4.吹扫、冲洗\n5.警示带铺设","m"]
[13,"铸铁管","1.名称、规格:柔性机制抗震铸铁管 DN50",null,"m"]
[14,"其他成品卫生器具","1.名称、规格：清扫口DN100 ","1.器具安装\n2.附件安装","组"]
[15,"塑料管","1.材质、规格:热水DN15","1.管道安装\n2.管件安装\n3.塑料卡固定\n4.阻火圈安装\n5.压力试验\n6.吹扫、冲洗\n7.警示带铺设","m"]
[16,"塑料管","1.材质、规格:热水DN20",null,"m"]
[17,"水表","1.名称、规格：水表 DN32","1.组装","组"]
[18,"洗脸盆","1.名称、规格：台式洗脸盆","1.器具安装\n2.附件安装","组"]
[19,"大便器","1.名称、规格：坐便器",null,"组"]
["报价合计",{"$nulls":13},0]

{"sheet":"预留用房-采暖","index":28,"n_rows":12,"n_cols":16,"rows_kept":12,"merged":[[0,0,0,15],[1,0,1,2],[1,4,1,7],[3,3,9,3],[11,0,11,13]],"flags":["formulas_cached_only"]}
["工程量清单报价表"]
["工程名称：预留用房-采暖"]
["序号","项目名称","项目特征描述","工作内容","单位","工程量","人工费（元）","辅材费（元）","机械费（元）","管理费（元）","利润（元）","不含税单价（元）","税率（3%）","含税单价\n（元）","含税合价\n（元）","备注"]
[1,"镀锌钢管","1.材质、规格:热镀锌钢管 DN20","1.管道安装\n2.管件制作、安装\n3.压力试验\n4.吹扫、冲洗\n5.警示带铺设","m"]
[2,"镀锌钢管","1.材质、规格:热镀锌钢管 DN25",null,"m"]
[3,"镀锌钢管","1.材质、规格:热镀锌钢管 DN32",null,"m"]
[4,"镀锌钢管","1.材质、规格:热镀锌钢管 DN40",null,"m"]
[5,"镀锌钢管","1.材质、规格:热镀锌钢管 DN50",null,"m"]
[6,"镀锌钢管","1.材质、规格:热镀锌钢管 DN65",null,"m"]
[7,"镀锌钢管","1.材质、规格:热镀锌钢管 DN80",null,"m"]
[8,"碳钢阀门","1.材质、规格:防火阀 160*120","1.阀体制作\n2.阀体安装\n3.支架制作、安装","个"]
["报价合计",{"$nulls":13},0]

{"sheet":"预留用房-电气","index":29,"n_rows":43,"n_cols":16,"rows_kept":43,"merged":[[0,0,0,15],[1,0,1,2],[1,4,1,7],[4,3,7,3],[9,3,11,3],[12,3,15,3],[21,3,25,3],[27,3,31,3],[32,3,36,3],[38,3,39,3],[42,0,42,13]],"flags":["formulas_cached_only"]}
["工程量清单报价表"]
["工程名称：预留用房-电气"]
["序号","项目名称","项目特征描述","工作内容","单位","工程量","人工费（元）","辅材费（元）","机械费（元）","管理费（元）","利润（元）","不含税单价（元）","税率（3%）","含税单价\n（元）","含税合价\n（元）","备注"]
[null,"电气部分"]
[1,"配电箱","1.名称、型号:1AL-500*600*200","1.本体安装\n2.基础型钢制作、安装\n3.焊、压接线端子\n4.补刷（喷)油漆\n5.接地","台"]
[2,"配电箱","1.名称、型号:2AL-500*600*200",null,"台"]
[3,"配电箱","1.名称、型号:2AL-1-300*200*100",null,"台"]
[4,"配电箱","1.名称、型号:AL701-600*800*250",null,"台"]
[5,"电力电缆","1.名称、型号:ZR-YJV-5*10","1.电缆敷设\n2.揭（盖）盖板","m"]
[6,"配线","1.名称、型号:ZN-RVSP-2*2.5","1.配线\n2.钢索架设（拉紧装置安装）\n3.支持体（夹板、绝缘子、槽板等)安装","m"]
[7,"配线","1.名称、型号:ZR-BV2.5",null,"m"]
[8,"配线","1.名称、型号:ZR-BV4",null,"m"]
[9,"配管","1.名称、型号:PVC20","1.电线管路敷设\n2.钢索架设（拉紧装置安装）\n3.预留沟槽\n4.接地","m"]
[10,"配管","1.名称、型号:PVC25",null,"m"]
[11,"配管","1.名称、型号:SC15",null,"m"]
[12,"配管","1.名称、型号:SC40",null,"m"]
[13,"电缆槽盒","1.名称、型号:弱电  100*75","1.槽盒安装","m"]
[14,"信息插座","1.名称、型号:电话插座-86型-RJ11","1.端接模块\n2.安装面板","个"]
[15,"普通灯具","1.名称、型号;防水防尘吸顶灯-~220V 1X18W","1.本体安装","套"]
[16,"小电器","1.名称、型号:风速开关-~220V 2X30W","1.本体安装\n2.焊、压接线端子\n3.接线","个"]
[17,"光纤配线架","1.名称、型号:光纤配线架","1.底座制作、安装\n2.本体安装、测试\n3.接地\n4.连接\n5.标识\n6.运输","架"]
[18,"装饰灯","1.名称、型号:楼层标志灯-A型灯具,DC36V 1W","1.本体安装","套"]
[19,"普通灯具","1.名称、型号;声光控开关吸顶灯-~220V 1X18W",null,"套"]
[20,"普通灯具","1.名称、型号;室外壁灯-~220V 1X18W",null,"套"]
[21,"普通灯具","1.名称、型号;室外雨棚灯-~220V 1X18W",null,"套"]
[22,"荧光灯","1.名称、型号:双管节能荧光灯-~220V 2X30W",null,"套"]
[23,"信息插座","1.名称、型号:信息插座-220V 36W","1.端接模块\n2.安装面板","个"]
[24,"装饰灯","1.名称、型号:应急疏散安全出口标志灯-A型灯具,DC36V 1W","1.本体安装","套"]
[25,"装饰灯","1.名称、型号:应急疏散疏散出口标志灯-A型灯具,DC36V 1W",null,"套"]
[26,"装饰灯","1.名称、型号:应急疏散指示标识灯-A型灯具,DC36V 1W",null,"套"]
[27,"装饰灯","1.名称、型号:应急照明灯壁装型-A型灯具,DC36V 1W",null,"套"]
[28,"普通灯具","1.名称、型号;坐灯头-~220V 1X18W",null,"套"]
[29,"小电器","1.名称、型号:单联单控开关","1.本体安装\n2.焊、压接线端子\n3.接线","个"]
[30,"小电器","1.名称、型号:单联防水密闭开关-~220V 10A",null,"个"]
[31,"小电器","1.名称、型号:二、三极安全型插座",null,"个"]
[32,"小电器","1.名称、型号:双联单控开关",null,"个"]
[33,"小电器","1.名称、型号:双联防水密闭开关-~220V 10A",null,"个"]
[null,"防雷接地"]
[33,"配电箱","1.名称、型号:局部等电位端子箱","1.本体安装\n2.基础型钢制作、安装\n3.焊、压接线端子\n4.补刷（喷)油漆\n5.接地","台"]
[34,"配电箱","1.名称、型号:总等电位端子箱",null,"台"]
[35,"接地母线","1.名称、型号:不锈钢接地线(M）--40X4","1.接地母线制作、安装\n2.补刷（喷)油漆","m"]
[36,"接地极","1.名称、型号:镀锌钢管接地极(根）-SC50  L=2.5米","1.接地极（板、桩)制作、安装\n2.基础接地网安装\n3.补刷（喷)油漆","根"]
["报价合计",{"$nulls":13},0]

{"sheet":"预留用房-给排水","index":30,"n_rows":39,"n_cols":16,"rows_kept":39,"merged":[[0,0,0,15],[1,0,1,2],[1,4,1,7],[3,3,11,3],[14,3,21,3],[23,3,26,3],[27,3,30,3],[34,3,35,3],[38,0,38,13]],"flags":["formulas_cached_only"]}
["工程量清单报价表"]
["工程名称：预留用房-给排水"]
["序号","项目名称","项目特征描述","工作内容","单位","工程量","人工费（元）","辅材费（元）","机械费（元）","管理费（元）","利润（元）","不含税单价（元）","税率(3%)","含税单价\n（元）","含税合价\n（元）","备注"]
[1,"螺纹阀门","1.名称、规格：减压阀 DN25","1.安装\n2.电气接线\n3.调试","个"]
[2,"螺纹阀门","1.名称、规格：闸阀 DN15",null,"个"]
[3,"螺纹阀门","1.名称、规格：闸阀 DN20",null,"个"]
[4,"螺纹阀门","1.名称、规格：闸阀 DN25",null,"个"]
[5,"螺纹阀门","1.名称、规格：闸阀 DN32",null,"个"]
[6,"螺纹阀门","1.名称、规格：闸阀 DN50",null,"个"]
[7,"螺纹阀门","1.名称、规格：闸阀 DN80",null,"个"]
[8,"螺纹阀门","1.名称、规格：止回阀 DN80",null,"个"]
[9,"螺纹阀门","1.名称、规格：自动排气阀 DN25",null,"个"]
[10,"其他成品卫生器具","1.名称、规格：地漏 DN50","1.器具安装\n2.附件安装","组"]
[11,"大便器","1.名称、规格：蹲便器","1.器具安装\n2.附件安装","组"]
[12,"复合管","1.名称、规格：内涂塑钢管（内涂聚乙烯PE) DN15","1.管道安装\n2.管件安装\n3.塑料卡固定\n4.压力试验\n5.吹扫、冲洗\n6.警示带铺设","m"]
[13,"复合管","1.名称、规格：内涂塑钢管（内涂聚乙烯PE) DN20",null,"m"]
[14,"复合管","1.名称、规格：内涂塑钢管（内涂聚乙烯PE) DN25",null,"m"]
[15,"复合管","1.名称、规格：内涂塑钢管（内涂聚乙烯PE) DN32",null,"m"]
[16,"复合管","1.名称、规格：内涂塑钢管（内涂聚乙烯PE) DN40",null,"m"]
[17,"复合管","1.名称、规格：内涂塑钢管（内涂聚乙烯PE) DN50",null,"m"]
[18,"复合管","1.名称、规格：内涂塑钢管（内涂聚乙烯PE) DN70",null,"m"]
[19,"复合管","1.名称、规格：内涂塑钢管（内涂聚乙烯PE) DN80",null,"m"]
[20,"淋浴器","1.名称、规格：淋浴器","1.器具安装\n2.附件安装","套"]
[21,"铸铁管","1.名称、规格:柔性机制抗震铸铁管 DN100","1.管道安装\n2.管件安装\n3.压力试验\n4.吹扫、冲洗\n5.警示带铺设","m"]
[22,"铸铁管","1.名称、规格:柔性机制抗震铸铁管 DN50",null,"m"]
[23,"铸铁管","1.名称、规格:柔性机制抗震铸铁管 DN70",null,"m"]
[24,"铸铁管","1.名称、规格:柔性机制抗震铸铁管 DN80",null,"m"]
[25,"塑料管","1.材质、规格:热水DN15","1.管道安装\n2.管件安装\n3.塑料卡固定\n4.阻火圈安装\n5.压力试验\n6.吹扫、冲洗\n7.警示带铺设","m"]
[26,"塑料管","1.材质、规格:热水DN20",null,"m"]
[27,"塑料管","1.材质、规格:热水DN25",null,"m"]
[28,"塑料管","1.材质、规格:热水DN50",null,"m"]
[29,"水表","1.名称、规格：水表 DN80","1.组装","组"]
[30,"洗脸盆","1.名称、规格：台式洗脸盆","1.器具安装\n2.附件安装","组"]
[31,"套管","1.名称、规格：刚性防水套管 DN80","1.制作\n2.安装\n3.除锈、刷油","个"]
[32,"洗涤盆","1.规格、类型:拖布池","1.器具安装\n2.附件安装","组"]
[33,"小便器","1.规格、类型:小便器",null,"组"]
[34,"螺纹阀门","1.名称、规格：真空破坏器 DN25","1.安装\n2.电气接线\n3.调试","个"]
[35,"大便器","1.名称、规格：坐便器","1.器具安装\n2.附件安装","组"]
["报价合计",{"$nulls":13},0]

{"sheet":"原水提升泵房-采暖","index":31,"n_rows":11,"n_cols":16,"rows_kept":11,"merged":[[0,0,0,15],[1,0,1,2],[1,4,1,7],[3,3,4,3],[5,3,8,3],[10,0,10,13]],"flags":["formulas_cached_only"]}
["工程量清单报价表"]
["工程名称：原水提升泵房-采暖"]
["序号","项目名称","项目特征描述","工作内容","单位","工程量","人工费（元）","辅材费（元）","机械费（元）","管理费（元）","利润（元）","不含税单价（元）","税率（3%）","含税单价\n（元）","含税合价\n（元）","备注"]
[1,"镀锌钢管","1.材质、规格:热镀锌钢管 DN20","1.管道安装\n2.管件制作、安装\n3.压力试验\n4.吹扫、冲洗\n5.警示带铺设","m"]
[2,"镀锌钢管","1.材质、规格:热镀锌钢管 DN25",null,"m"]
[3,"螺纹阀门","1.材质、规格:温控阀 DN20","1.安装\n2.电气接线\n3.调试","个"]
[4,"螺纹阀门","1.材质、规格:截止阀J11T-10 DN20",null,"个"]
[5,"螺纹阀门","1.材质、规格:排气阀 DN20",null,"个"]
[6,"螺纹阀门","1.材质、规格:手动调节阀 DN25",null,"个"]
[7,"钢制散热器","1.材质、规格:钢制散热器（UR7002-600）25片","1.安装\n2.托架安装\n3.托架刷油","组"]
["报价合计",{"$nulls":13},0]

{"sheet":"原水提升泵房-电气","index":32,"n_rows":21,"n_cols":16,"rows_kept":21,"merged":[[0,0,0,15],[1,0,1,2],[1,4,1,7],[5,3,6,3],[7,3,8,3],[10,3,12,3],[13,3,14,3],[17,3,18,3],[20,0,20,13]],"flags":["formulas_cached_only"]}
["工程量清单报价表"]
["工程名称：原水提升泵房-电气"]
["序号","项目名称","项目特征描述","工作内容","单位","工程量","人工费（元）","辅材费（元）","机械费（元）","管理费（元）","利润（元）","不含税单价（元）","税率（3%）","含税单价\n（元）","含税合价\n（元）","备注"]
[null,"电气"]
[1,"配电箱","1.名称、型号:AL1301-450*600*180","1.本体安装\n2.基础型钢制作、安装\n3.焊、压接线端子\n4.补刷（喷)油漆\n5.接地","台"]
[2,"配线","1.名称、型号:ZR-BV2.5","1.配线\n2.钢索架设（拉紧装置安装）\n3.支持体（夹板、绝缘子、槽板等)安装","m"]
[3,"配线","1.名称、型号:ZR-BV4",null,"m"]
[4,"配管","1.名称、型号:PVC20","1.电线管路敷设\n2.钢索架设（拉紧装置安装）\n3.预留沟槽\n4.接地","m"]
[5,"配管","1.名称、型号:PVC25",null,"m"]
[6,"电缆槽盒","1.名称、型号:镀锌槽式电缆桥架 200X100","1.槽盒安装","m"]
[7,"普通灯具","1.名称、型号;防水防尘吸顶灯-~220V 1X18W","1.本体安装","套"]
[8,"普通灯具","1.名称、型号:吸顶灯-~220V 1X18W",null,"套"]
[9,"装饰灯","1.名称、型号:自带蓄电池双管节能荧光灯-~220V 2X30W",null,"套"]
[10,"小电器","1.名称、型号:二、三极安全型插座","1.本体安装\n2.焊、压接线端子\n3.接线","个"]
[11,"小电器","1.名称、型号:三联防水密闭开关",null,"个"]
[null,"防雷接地"]
[12,"配电箱","1.名称、型号:总等电位端子箱（台）-TD28","1.本体安装\n2.基础型钢制作、安装\n3.焊、压接线端子\n4.补刷（喷)油漆\n5.接地","台"]
[13,"接地母线","1.名称、型号:不锈钢接地线（M）-40X4","1.接地母线制作、安装\n2.补刷（喷)油漆","m"]
[14,"接地母线","1.名称、型号:镀锌扁钢接地线（M)--40X4",null,"m"]
[15,"接地极","1.名称、型号:镀锌钢管接地极（根）-SC50  L=2.5米","1.接地极（板、桩)制作、安装\n2.基础接地网安装\n3.补刷（喷)油漆","根"]
["报价合计",{"$nulls":13},0]

{"sheet":"综合水池及泵房-采暖","index":33,"n_rows":11,"n_cols":16,"rows_kept":11,"merged":[[0,0,0,15],[1,0,1,2],[1,4,1,7],[3,3,4,3],[5,3,8,3],[10,0,10,13]],"flags":["formulas_cached_only"]}
["工程量清单报价表"]
["工程名称：综合水池及泵房-采暖"]
["序号","项目名称","项目特征描述","工作内容","单位","工程量","人工费（元）","辅材费（元）","机械费（元）","管理费（元）","利润（元）","不含税单价（元）","税率（3%）","含税单价\n（元）","含税合价\n（元）","备注"]
[1,"镀锌钢管","1.材质、规格:热镀锌钢管 DN20","1.管道安装\n2.管件制作、安装\n3.压力试验\n4.吹扫、冲洗\n5.警示带铺设","m"]
[2,"镀锌钢管","1.材质、规格:热镀锌钢管 DN25",null,"m"]
[3,"螺纹阀门","1.材质、规格:温控阀 DN20","1.安装\n2.电气接线\n3.调试","个"]
[4,"螺纹阀门","1.材质、规格:截止阀J11T-10 DN20",null,"个"]
[5,"螺纹阀门","1.材质、规格:排气阀 DN20",null,"个"]
[6,"螺纹阀门","1.材质、规格:手动调节阀 DN25",null,"个"]
[7,"钢制散热器","1.材质、规格:钢制散热器（UR7002-600）25片","1.安装\n2.托架安装\n3.托架刷油","组"]
["报价合计",{"$nulls":13},0]

{"sheet":"综合水池及泵房-电气","index":34,"n_rows":28,"n_cols":16,"rows_kept":28,"merged":[[0,0,0,15],[1,0,1,2],[1,4,1,7],[4,3,9,3],[12,3,13,3],[14,3,18,3],[20,3,21,3],[24,3,25,3],[27,0,27,13]],"flags":["formulas_cached_only"]}
["工程量清单报价表"]
["工程名称：综合水池及泵房-电气"]
["序号","项目名称","项目特征描述","工作内容","单位","工程量","人工费（元）","辅材费（元）","机械费（元）","管理费（元）","利润（元）","不含税单价（元）","税率（3%）","含税单价\n（元）","含税合价\n（元）","备注"]
[null,"电气"]
[1,"配电箱","1.名称、型号:AL1301-450*600*180ALE-300*200*150","1.安装\n2.托架安装\n3.托架刷油","台"]
[2,"配电箱","1.名称、型号:FJX1101-400*500*250",null,"台"]
[3,"配电箱","1.名称、型号:电动葫芦配电箱",null,"台"]
[4,"配电箱","1.名称、型号:动力配电柜-800*600*2200",null,"台"]
[5,"配电箱","1.名称、型号:检修配电箱-450*600*200",null,"台"]
[6,"配电箱","1.名称、型号:水泵动力配电箱-450*600*250",null,"台"]
[7,"电力电缆","1.名称、型号:ZR-YJV-4*2.5","1.电缆敷设\n2.揭（盖）盖板","m"]
[8,"配线","1.名称、型号:ZN-RVSP-2X2.5","1.配线\n2.钢索架设（拉紧装置安装）\n3.支持体（夹板、绝缘子、槽板等)安装","m"]
[9,"配管","1.名称、型号:SC15","1.电线管路敷设\n2.钢索架设（拉紧装置安装）\n3.预留沟槽\n4.接地","m"]
[10,"配管","1.名称、型号:SC25",null,"m"]
[11,"普通灯具","1.名称、型号;防水防尘吸顶灯(自带蓄电池)-~220V 1X24W","1.本体安装","套"]
[12,"装饰灯","1.名称、型号:声光控开关吸顶灯-~220V 1X18W",null,"套"]
[13,"装饰灯","1.名称、型号:疏散出口标志灯-A型灯具,DC36V 1W",null,"套"]
[14,"装饰灯","1.名称、型号:应急疏散指示标识灯-A型灯具,DC36V 1W",null,"套"]
[15,"装饰灯","1.名称、型号:应急照明灯壁装型-A型灯具,DC36V 5W",null,"套"]
[16,"小电器","1.名称、型号:防水二联单控开关","1.本体安装\n2.焊、压接线端子\n3.接线","个"]
[17,"电缆槽盒","1.名称、型号:电缆桥架(M）-200*100","1.槽盒安装","m"]
[18,"电缆槽盒","1.名称、型号:电缆桥架(M）-200*200",null,"m"]
[null,"防雷接地"]
[19,"配电箱","1.名称、型号:总等电位端子箱（台）-TD28","1.本体安装\n2.基础型钢制作、安装\n3.焊、压接线端子\n4.补刷（喷)油漆\n5.接地","台"]
[20,"接地母线","1.名称、型号:不锈钢接地线（M）-40X4","1.接地母线制作、安装\n2.补刷（喷)油漆","m"]
[21,"接地母线","1.名称、型号:镀锌扁钢接地线（M)--40X4",null,"m"]
[22,"接地极","1.名称、型号:镀锌钢管接地极（根）-SC50  L=2.5米","1.接地极（板、桩)制作、安装\n2.基础接地网安装\n3.补刷（喷)油漆","根"]
["报价合计",{"$nulls":13},0]

{"sheet":"综合水池及泵房-给排水","index":35,"n_rows":17,"n_cols":16,"rows_kept":17,"merged":[[0,0,0,15],[1,0,1,2],[1,4,1,7],[4,3,5,3],[9,3,10,3],[11,3,12,3],[16,0,16,13]],"flags":["formulas_cached_only"]}
["工程量清单报价表"]
["工程名称：综合水池及泵房-给排水"]
["序号","项目名称","项目特征描述","工作内容","单位","工程量","人工费（元）","辅材费（元）","机械费（元）","管理费（元）","利润（元）","不含税单价（元）","税率（3%）","含税单价\n（元）","含税合价\n（元）","备注"]
[null,"给水"]
[1,"焊接法兰阀门","1.名称、规格：闸阀 DN100","1.安装\n2.电气接线\n3.调试","个"]
[2,"焊接法兰阀门","1.名称、规格：Y型过滤器 DN100",null,"个"]
[3,"复合管","1.名称、规格：内涂塑钢管（内涂聚乙烯PE) DN100","1.管道安装\n2.管件安装\n3.塑料卡固定\n4.压力试验\n5.吹扫、冲洗\n6.警示带铺设","m"]
[4,"套管","1.名称、规格：刚性防水套管 DN100","1.制作\n2.安装\n3.除锈、刷油","个"]
[null,"废水"]
[5,"焊接法兰阀门","1.名称、规格：铜芯闸阀 DN50","1.安装\n2.电气接线\n3.调试","个"]
[6,"焊接法兰阀门","1.名称、规格：止回阀 DN50",null,"个"]
[7,"复合管","1.名称、规格：涂塑镀锌钢管 DN50","1.管道安装\n2.管件安装\n3.塑料卡固定\n4.压力试验\n5.吹扫、冲洗\n6.警示带铺设","m"]
[8,"复合管","1.名称、规格：涂塑镀锌钢管 DN70",null,"m"]
[9,"离心式泵","1.名称:潜污泵","1.本体安装\n2.泵拆装检查\n3.电动机安装\n4.二次灌装\n5.单机试运转\n6.补刷（喷)油漆","台"]
[10,"套管","1.名称、规格：刚性防水套管 DN70","1.制作\n2.安装\n3.除锈、刷油","个"]
[11,"压力仪表","1.名称、规格：压力表 DN50","1.本体安装\n2.压力表弯制作、安装\n3.挠性管安装\n4.取源部件配合安装\n5.单体校验调整\n6.脱脂\n7.支架制作、安装","台"]
["报价合计",{"$nulls":13},0]

{"sheet":"综合用房-采暖","index":36,"n_rows":15,"n_cols":16,"rows_kept":15,"merged":[[0,0,0,15],[1,0,1,2],[1,4,1,8],[3,3,7,3],[8,3,10,3],[11,3,13,3],[14,0,14,13]],"flags":["formulas_cached_only"]}
["工程量清单报价表"]
["工程名称：综合用房-采暖"]
["序号","项目名称","项目特征描述","工作内容","单位","工程量","人工费（元）","辅材费（元）","机械费（元）","管理费（元）","利润（元）","不含税单价（元）","税率（3%）","含税单价\n（元）","含税合价\n（元）","备注"]
[1,"镀锌钢管","1.材质、规格:热镀锌钢管 DN25","1.管道安装\n2.管件制作、安装\n3.压力试验\n4.吹扫、冲洗\n5.警示带铺设","m"]
[2,"镀锌钢管","1.材质、规格:热镀锌钢管 DN32",null,"m"]
[3,"镀锌钢管","1.材质、规格:热镀锌钢管 DN40",null,"m"]
[4,"镀锌钢管","1.材质、规格:热镀锌钢管 DN50",null,"m"]
[5,"镀锌钢管","1.材质、规格:热镀锌钢管 DN65",null,"m"]
[6,"螺纹阀门","1.材质、规格:手动调节阀 DN20","1.安装\n2.电气接线\n3.调试","个"]
[7,"螺纹阀门","1.材质、规格:闸阀 DN20",null,"个"]
[8,"螺纹阀门","1.材质、规格:自动排气阀 DN20",null,"个"]
[9,"钢制散热器","1.材质、规格:钢制散热器（UR7002-600）20片","1.安装\n2.托架安装\n3.托架刷油","组"]
[10,"钢制散热器","1.材质、规格:钢制散热器（UR7002-600）24片",null,"组"]
[11,"钢制散热器","1.材质、规格:钢制散热器（UR7002-600）25片",null,"组"]
["报价合计",{"$nulls":13},0]

{"sheet":"综合用房-电气","index":37,"n_rows":83,"n_cols":16,"rows_kept":83,"merged":[[0,0,0,15],[1,0,1,2],[1,4,1,7],[4,3,5,3],[6,3,9,3],[10,3,11,3],[13,3,18,3],[19,3,23,3],[24,3,31,3],[32,3,33,3],[34,3,41,3],[43,3,45,3],[48,3,58,3],[59,3,62,3],[63,3,64,3],[65,3,73,3],[77,3,79,3],[82,0,82,13]],"flags":["formulas_cached_only"]}
["工程量清单报价表"]
["工程名称：综合用房-电气"]
["序号","项目名称","项目特征描述","工作内容","单位","工程量","人工费（元）","辅材费（元）","机械费（元）","管理费（元）","利润（元）","不含税单价（元）","税率（3%）","含税单价\n（元）","含税合价\n（元）","备注"]
[null,"动力部分"]
[1,"低压开关柜","1.名称、型号:低压配电柜\n2.规格:1000*800*2200","1.基础型钢制作、安装\n2.本体安装、单体调试\n3.接地\n4.运输","台"]
[2,"低压开关柜","1.名称、型号:低压配电柜（远期预留）\n2.规格:1000*800*2200",null,"台"]
[3,"配电箱","1.名称、型号:机修车间动力箱 JXF 506020","1.本体安装\n2.基础型钢制作、安装\n3.焊、压接线端子\n4.补刷（喷)油漆\n5.接地","台"]
[4,"配电箱","1.名称、型号:综合用房照明配电箱\n2.规格:400*500*200",null,"台"]
[5,"配电箱","1.名称、型号:综合用房检修配电箱 JXF 405020",null,"台"]
[6,"配电箱","1.名称、型号:综合用房风机配电箱 JXF506020",null,"台"]
[7,"电缆槽盒","1.名称、型号:镀锌槽式电缆桥架 300X100","1.槽盒安装","m"]
[8,"电缆槽盒","1.名称、型号:镀锌槽式电缆桥架200X100",null,"m"]
[9,"铺砂、盖保护板(砖）","1.名称、型号:电缆沟 800X1000","1.铺砂\n2.盖板(砖）","m"]
[10,"装饰灯","1.名称、型号:LED投光灯-LED 防尘防水型 50W","1.本体安装","套"]
[11,"装饰灯","1.名称、型号:自带蓄电池T8双管 LED 2X22W",null,"套"]
[12,"装饰灯","1.名称、型号:自带蓄电池T8单管 LED 22W",null,"套"]
[13,"装饰灯","1.名称、型号:T8双管LED灯 LED 2x22W",null,"套"]
[14,"普通灯具","1.名称、型号:圆形吸顶灯 LED 25W",null,"套"]
[15,"装饰灯","1.名称、型号:天棚灯-LED 18W",null,"套"]
[16,"小电器","1.名称、型号:单联开关-86K11-10","1.本体安装\n2.焊、压接线端子\n3.接线","个"]
[17,"小电器","1.名称、型号:双联开关-86K21-10",null,"个"]
[18,"小电器","1.名称、型号:三联开关-86K31-10",null,"个"]
[19,"小电器","1.名称、型号:安全型单相五孔暗装插座-86Z23-10",null,"个"]
[20,"小电器","1.名称、型号:空调专用接线开关 220V 25A",null,"个"]
[21,"电力电缆","1.名称、型号:YJV-0.6/1KV-3*95+2*50","1.电缆敷设\n2.揭（盖）盖板","m"]
[22,"电力电缆","1.名称、型号:YJV-0.6/1KV-3*185+2*95",null,"m"]
[23,"电力电缆","1.名称、型号:YJV-0.6/1KV-3*35+2*16",null,"m"]
[24,"电力电缆","1.名称、型号:YJV-0.6/1KV-5*10",null,"m"]
[25,"电力电缆","1.名称、型号:YJV-0.6/1KV-5*6",null,"m"]
[26,"电力电缆","1.名称、型号:YJV-0.6/1KV-5*4",null,"m"]
[27,"电力电缆","1.名称、型号:YJV-0.6/1KV-5*16",null,"m"]
[28,"电力电缆","1.名称、型号:YJV-4x4",null,"m"]
[29,"配线","1.名称、型号:ZR-BV2.5","1.配线\n2.钢索架设（拉紧装置安装）\n3.支持体（夹板、绝缘子、槽板等)安装","m"]
[30,"配线","1.名称、型号:ZR-BV4",null,"m"]
[31,"配管","1.名称、型号:SC80","1.电线管路敷设\n2.钢索架设（拉紧装置安装）\n3.预留沟槽\n4.接地","m"]
[32,"配管","1.名称、型号:SC65",null,"m"]
[33,"配管","1.名称、型号:SC50",null,"m"]
[34,"配管","1.名称、型号:SC32",null,"m"]
[35,"配管","1.名称、型号:SC20",null,"m"]
[36,"配管","1.名称、型号:PVC20",null,"m"]
[37,"配管","1.名称、型号:PVC25",null,"m"]
[38,"配管","1.名称、型号:SC20",null,"m"]
[39,"配电箱","1.名称、型号:等电位端子箱 TD28","1.本体安装\n2.基础型钢制作、安装\n3.焊、压接线端子\n4.补刷（喷)油漆\n5.接地","台"]
[40,"接地母线","1.名称、型号:镀锌扁钢接地线 -40X4","1.接地母线制作、安装\n2.补刷（喷)油漆","m"]
[41,"接地母线","1.名称、型号:接地保护连接线 -25X4 镀锌扁铁",null,"m"]
[42,"接地母线","1.名称、型号:接地保护连接线 -40X4 不锈钢扁铁",null,"m"]
[43,"接地极","1.名称、型号:接地极-Φ50镀锌钢管长2500MM","1.接地极（板、桩)制作、安装\n2.基础接地网安装\n3.补刷（喷)油漆","根"]
[null,"照明部分"]
[44,"装饰灯","1.名称、型号:A型安全出口标志灯-1X1W  36V","1.本体安装","套"]
[45,"装饰灯","1.名称、型号:A型双向疏散指示灯-1X1W  36V",null,"套"]
[46,"装饰灯","1.名称、型号:A型应急照明灯-5W  36V",null,"套"]
[47,"装饰灯","1.名称、型号:A型应急照明灯(壁装型)-5W  36V 室外IP67",null,"套"]
[48,"装饰灯","1.名称、型号:A型右向疏散指示灯-1X1W  36V",null,"套"]
[49,"装饰灯","1.名称、型号:A型左向疏散指示灯-1X1W  36V",null,"套"]
[50,"工厂灯","1.名称、型号:LED工厂灯-LED 广照型 100W 带遥控升降器",null,"套"]
[51,"装饰灯","1.名称、型号:LED投光灯-LED 防尘防水型 40W",null,"套"]
[52,"装饰灯","1.名称、型号:天棚灯-LED 18W",null,"套"]
[53,"装饰灯","1.名称、型号:自带蓄电池T8单管LED灯-LED 22W",null,"套"]
[54,"装饰灯","1.名称、型号:自带蓄电池T8双管LED灯-LED 2X22W",null,"套"]
[55,"小电器","1.名称、型号:安全型单相五孔暗装插座-86Z23-10","1.本体安装\n2.焊、压接线端子\n3.接线","个"]
[56,"小电器","1.名称、型号:空调专用插座",null,"个"]
[57,"小电器","1.名称、型号:三联开关-86K31-10",null,"个"]
[58,"小电器","1.名称、型号:双联开关-86K21-10",null,"个"]
[59,"配线","1.名称、型号:NH-BV2.5","1.配线\n2.钢索架设（拉紧装置安装）\n3.支持体（夹板、绝缘子、槽板等)安装","m"]
[60,"配线","1.名称、型号:ZR-BV4",null,"m"]
[61,"配管","1.名称、型号:PVC25","1.电线管路敷设\n2.钢索架设（拉紧装置安装）\n3.预留沟槽\n4.接地","m"]
[62,"配管","1.名称、型号:SC100",null,"m"]
[63,"配管","1.名称、型号:SC125",null,"m"]
[64,"配管","1.名称、型号:SC20",null,"m"]
[65,"配管","1.名称、型号:SC25",null,"m"]
[66,"配管","1.名称、型号:SC32",null,"m"]
[67,"配管","1.名称、型号:SC50",null,"m"]
[68,"配管","1.名称、型号:SC65",null,"m"]
[69,"配管","1.名称、型号:SC80",null,"m"]
[null,"防雷接地"]
[70,"接闪器支架","1.名称、型号:接闪器支架-Φ12热镀锌圆钢300MM","1.避雷网制作、安装\n2.跨接\n3.混凝土块制作\n4.补刷（喷)油漆","m"]
[71,"避雷引下线","1.名称、型号:防雷引下线-利用主框架柱内钢筋","1.避雷引下线制作、安装\n2.断接卡子、箱制作、安装\n3.利用主钢筋焊接\n4.补刷（喷)油漆","处"]
[72,"接地母线","1.名称、型号:桥架接地保护连接线--25X4 镀锌扁铁","1.接地母线制作、安装\n2.补刷（喷)油漆","m"]
[73,"接地母线","1.名称、型号:室外接地保护连接线--40X4不锈钢扁铁",null,"m"]
[74,"接地母线","1.名称、型号:等电位连接线--40X4",null,"m"]
[75,"避雷网","1.名称、型号:接闪带-Φ12热镀锌圆钢","1.避雷网制作、安装\n2.跨接\n3.混凝土块制作\n4.补刷（喷)油漆","m"]
[76,"接地极","1.名称、型号:接地极-Φ50镀锌钢管长2500MM","1.接地极（板、桩)制作、安装\n2.基础接地网安装\n3.补刷（喷)油漆","根"]
["报价合计",{"$nulls":13},0]

{"sheet":"综合用房-给排水","index":38,"n_rows":13,"n_cols":16,"rows_kept":13,"merged":[[0,0,0,15],[1,0,1,2],[1,4,1,7],[3,3,6,3],[7,3,9,3],[12,0,12,13]],"flags":["formulas_cached_only"]}
["工程量清单报价表"]
["工程名称：综合用房-给排水"]
["序号","项目名称","项目特征描述","工作内容","单位","工程量","人工费（元）","辅材费（元）","机械费（元）","管理费（元）","利润（元）","不含税单价（元）","税率（3%）","含税单价\n（元）","含税合价\n（元）","备注"]
[1,"螺纹阀门","1.名称、规格：减压阀 DN50","1.安装\n2.电气接线\n3.调试","个"]
[2,"螺纹阀门","1.名称、规格：截止阀 DN25",null,"个"]
[3,"螺纹阀门","1.名称、规格：闸阀 DN50",null,"个"]
[4,"螺纹阀门","1.名称、规格：真空破坏器 DN25",null,"个"]
[5,"复合管","1.名称、规格：内涂塑钢管（内涂聚乙烯PE) DN25","1.管道安装\n2.管件安装\n3.塑料卡固定\n4.压力试验\n5.吹扫、冲洗\n6.警示带铺设","m"]
[6,"复合管","1.名称、规格：内涂塑钢管（内涂聚乙烯PE) DN32",null,"m"]
[7,"复合管","1.名称、规格：内涂塑钢管（内涂聚乙烯PE) DN50",null,"m"]
[8,"水表","1.名称、规格：水表 DN25","1.组装","组"]
[9,"套管","1.名称、规格：刚性防水套管 DN50","1.制作\n2.安装\n3.除锈、刷油","个"]
["报价合计",{"$nulls":13},0]

{"sheet":"室外-电气工程","index":39,"n_rows":12,"n_cols":16,"rows_kept":12,"merged":[[0,0,0,15],[1,0,1,2],[1,4,1,7],[3,3,4,3],[6,3,8,3],[9,3,10,3],[11,0,11,13]],"flags":["formulas_cached_only"]}
["工程量清单报价表"]
["工程名称：室外-电气"]
["序号","项目名称","项目特征描述","工作内容","单位","工程量","人工费（元）","辅材费（元）","机械费（元）","管理费（元）","利润（元）","不含税单价（元）","税率3%","含税单价\n（元）","含税合价\n（元）","备注"]
[1,"配电箱","1.名称、型号:除臭装置控制箱","1.本体安装\n2.基础型钢制作、安装\n3.焊、压接线端子\n4.补刷（喷)油漆\n5.接地","台",1]
[2,"配电箱","1.名称、型号:磅房及室外照明配电箱 JXF(400x500x200)",null,"台",1]
[3,"设备电缆、软光纤","1.名称、型号:四芯单模光纤","1.放绑\n2.编扎、焊（绕、卡）接\n3.试通","m",400]
[4,"电力电缆","1.名称、型号:ZC-YJV22-8.7/15-3x300","1.电缆敷设\n2.揭（盖）盖板","m",400]
[5,"电力电缆","1.名称、型号:YJV-0.6/1kV-3x6",null,"m",1300]
[6,"电力电缆","1.名称、型号:YJV-0.6/1kV-4x10",null,"m",760]
[7,"一般路灯","1.名称、型号:路灯 150W LED 杆高10米 钢制灯杆","1.立灯杆\n2.杆座安装\n3.灯架及灯具附件安装\n4.焊、压接线端子\n5.补刷（喷）油漆\n6.灯杆编号\n7.接地","套",26]
[8,"一般路灯","1.名称、型号:低杆路灯 60W LED 杆高6米 钢制灯杆",null,"套",67]
["报价合计",{"$nulls":13},0]

{"sheet":"室外-给排水工程","index":40,"n_rows":58,"n_cols":16,"rows_kept":58,"merged":[[0,0,0,15],[1,0,1,2],[1,4,1,7],[4,3,10,3],[11,3,17,3],[18,3,32,3],[33,3,38,3],[40,3,51,3],[53,3,56,3],[57,0,57,13]],"flags":["formulas_cached_only"]}
["工程量清单报价表"]
["工程名称：室外-给排水"]
["序号","项目名称","项目特征描述","工作内容","单位","工程量","人工费（元）","辅材费（元）","机械费（元）","管理费（元）","利润（元）","不含税单价（元）","税率（3%）","含税单价\n（元）","含税合价\n（元）","备注"]
[null,"给水"]
[1,"塑料管","1.名称、规格：PE100 1.0MPa DN150","1.管道安装\n2.管件安装\n3.塑料卡固定\n4.阻火圈安装\n5.压力试验\n6.吹扫、冲洗\n7.警示带铺设","m"]
[2,"塑料管","1.名称、规格：PE100 1.0MPa DN100",null,"m"]
[3,"塑料管","1.名称、规格：PE100 1.0MPa DN80",null,"m"]
[4,"塑料管","1.名称、规格：PE100 1.0MPa DN70",null,"m"]
[5,"塑料管","1.名称、规格：PE100 1.0MPa DN50",null,"m"]
[6,"塑料管","1.名称、规格：PE100 1.0MPa DN40",null,"m"]
[7,"塑料管","1.名称、规格：PE100 1.0MPa DN25",null,"m"]
[8,"水表","1.名称、规格：水表 DN40","1.组装","组"]
[12,"水表","1.名称、规格：水表 DN25",null,"组"]
[16,"水表","1.名称、规格：水表 DN50",null,"组"]
[20,"水表","1.名称、规格：水表 DN70",null,"组"]
[21,"水表","1.名称、规格：水表 DN80",null,"组"]
[28,"水表","1.名称、规格：水表 DN100",null,"组"]
[29,"水表","1.名称、规格：水表 DN150",null,"组"]
[9,"螺纹阀门","1.名称、规格：闸阀 DN40","1.安装\n2.电气接线\n3.调试","个"]
[10,"螺纹阀门","1.名称、规格：止回阀 DN40",null,"个"]
[11,"螺纹阀门","1.名称、规格：伸缩接头 DN40",null,"个"]
[13,"螺纹阀门","1.名称、规格：闸阀 DN25",null,"个"]
[14,"螺纹阀门","1.名称、规格：止回阀 DN25",null,"个"]
[15,"螺纹阀门","1.名称、规格：伸缩接头 伸缩接头 DN25",null,"个"]
[17,"螺纹阀门","1.名称、规格：蝶阀 DN50",null,"个"]
[18,"螺纹阀门","1.名称、规格：止回阀 DN50",null,"个"]
[19,"螺纹阀门","1.名称、规格：伸缩接头 DN50",null,"个"]
[22,"螺纹阀门","1.名称、规格：蝶阀 DN70",null,"个"]
[23,"螺纹阀门","1.名称、规格：蝶阀 DN80",null,"个"]
[24,"螺纹阀门","1.名称、规格：止回阀 DN70",null,"个"]
[25,"螺纹阀门","1.名称、规格：止回阀 DN80",null,"个"]
[26,"螺纹阀门","1.名称、规格：伸缩接头 DN70",null,"个"]
[27,"螺纹阀门","1.名称、规格：伸缩接头 DN80",null,"个"]
[30,"焊接法兰阀门","1.名称、规格：蝶阀 DN100","1.安装\n2.电气接线\n3.调试","个"]
[31,"焊接法兰阀门","1.名称、规格：蝶阀 DN150",null,"个"]
[32,"焊接法兰阀门","1.名称、规格：止回阀 DN100",null,"个"]
[33,"焊接法兰阀门","1.名称、规格：止回阀 DN150",null,"个"]
[34,"焊接法兰阀门","1.名称、规格：伸缩接头 DN100",null,"个"]
[35,"焊接法兰阀门","1.名称、规格：伸缩接头 DN150",null,"个"]
[null,"污水"]
[36,"承插水泥管","1.名称、规格：生活污水管 Ⅱ级钢筋混凝土管 DN100","1.管道安装\n2.管件安装\n3.压力试验\n4.吹扫、冲洗\n5.警示带铺设","m"]
[37,"承插水泥管","1.名称、规格：生活污水管 Ⅱ级钢筋混凝土管 DN150",null,"m"]
[38,"承插水泥管","1.名称、规格：生活污水管 Ⅱ级钢筋混凝土管 DN150",null,"m"]
[39,"承插水泥管","1.名称、规格：生活污水管 Ⅱ级钢筋混凝土管 DN200",null,"m"]
[40,"承插水泥管","1.名称、规格：污水管 Ⅱ级钢筋混凝土管 DN100",null,"m"]
[41,"承插水泥管","1.名称、规格：污水管 Ⅱ级钢筋混凝土管 DN150",null,"m"]
[42,"承插水泥管","1.名称、规格：污水管 Ⅱ级钢筋混凝土管 DN200",null,"m"]
[43,"承插水泥管","1.名称、规格：污水管 Ⅱ级钢筋混凝土管 DN250",null,"m"]
[44,"承插水泥管","1.名称、规格：污水管 Ⅱ级钢筋混凝土管 DN300",null,"m"]
[45,"承插水泥管","1.名称、规格：污水管 Ⅱ级钢筋混凝土管 DN350",null,"m"]
[46,"承插水泥管","1.名称、规格：污水管 Ⅱ级钢筋混凝土管 DN400",null,"m"]
[47,"铜管","1.名称、规格：不锈钢管 DN200",null,"m"]
[null,"雨水"]
[48,"承插水泥管","1.名称、规格：污水管 Ⅱ级钢筋混凝土管 DN300","1.管道安装\n2.管件安装\n3.压力试验\n4.吹扫、冲洗\n5.警示带铺设","m"]
[49,"承插水泥管","1.名称、规格：污水管 Ⅱ级钢筋混凝土管 DN400",null,"m"]
[50,"承插水泥管","1.名称、规格：污水管 Ⅱ级钢筋混凝土管 DN500",null,"m"]
[51,"承插水泥管","1.名称、规格：污水管 Ⅱ级钢筋混凝土管 DN800",null,"m"]
["报价合计",{"$nulls":13},0]